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               SAFETY DATA SHEET

 1. SUBSTANCE AND SOURCE IDENTIFICATION

Product Identifier
  SRM Number: 3147a
  SRM Name:   Samarium (Sm) Standard Solution
    Other Means of Identification: Not applicable.

Recommended Use of This Material and Restrictions of Use
    This Standard Reference Material (SRM) is intended for use as a primary calibration standard for the quantitative
    determination of samarium. A unit of SRM 3147a consists of five 10 mL sealed borosilicate glass ampoules of
    an acidified aqueous solution prepared gravimetrically to contain a known mass fraction of samarium.  The
    solution contains nitric acid at an amount-of-substance concentration (molarity) of approximately 1.6 mol/L.

Company Information

     National Institute of Standards and Technology
     Standard Reference Materials Program
     100 Bureau Drive, Stop 2300
      Gaithersburg, Maryland 20899-2300

     Telephone: 301-975-2200                         Emergency Telephone ChemTrec:
    FAX: 301-948-3730                                  1-800-424-9300   (North America)
     E-mail: SRMMSDS@nist.gov                        +1-703-527-3887    (International)
     Website: http://www.nist.gov/srm

 2. HAZARDS IDENTIFICATION

Classification
    Physical Hazard:    Not classified.
    Health Hazard:      Skin Corrosion/Irritation            Category 1B
                          Serious Eye Damage/Irritation       Category 1
    Label Elements
   Symbol





    Signal Word
   DANGER

   Hazard Statement(s)
   H314               Causes severe skin burns and eye damage.

    Precautionary Statement(s)
    P260            Do not breathe fumes, mists, vapors, or spray.
    P264             Wash hands thoroughly after handling.
    P280              Wear protective gloves, protective clothing, and eye protection.

    P301 + P330 + P331   If swallowed: Rinse mouth. Do NOT induce vomiting.
    P303 + P361 + P353   If on skin (or hair): Remove immediately all contaminated clothing.  Rinse skin with
                           water.
    P304 + P340             If inhaled: Remove person to fresh air and keep comfortable for breathing.
    P305 + P351 + P338   If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if
                           present and easy to do. Continue rinsing.
    P310                Immediately call a doctor.
    P363             Wash contaminated clothing before reuse.

    P405                  Store locked up.
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    P501                Dispose of contents and container according to local regulations.

   Hazards Not Otherwise Classified: Not applicable.

    Ingredients(s) with Unknown Acute Toxicity: Not applicable.

 3. COMPOSITION AND INFORMATION ON HAZARDOUS INGREDIENTS

Substance: Nitric acid/Samarium nitrate solution

Other Designations:
   Nitric acid (aqua fortis; hydrogen nitrate; azotic acid; engraver’s acid)
   Samarium nitrate (Samarium trinitrate)

NOTE: Samarium in nitric acid solution forms a solvated samarium nitrate salt. The health and physical hazard
information provided in this SDS are for nitric acid and samarium nitrate. No physical or chemical data are listed for
this solution. The actual effects of the solution may differ from the individual components.

Components are listed in compliance with OSHA’s 29 CFR 1910.1200; for the actual values see the Certificate of
Analysis.

 Hazardous Component(s)       CAS Number    EC Number     Nominal Mass Concentration
                                               (EINECS)               (%)
 Nitric acid                           7697-37-2         231-714-2                 10
 Samarium nitrate                     10361-83-8         233-798-6                     2.0

 Non-Hazardous Component(s)
 Water                               7732-18-5         231-791-2               >87


 4. FIRST AID MEASURES

Description of First Aid Measures:

    Inhalation:  If adverse effects occur, remove to uncontaminated area. If not breathing, give artificial respiration
    or oxygen by qualified personnel. Seek immediate medical attention.

    Skin Contact: Wash skin with soap and water for at least 15 minutes while removing contaminated clothing and
    shoes. Get immediate medical attention. Thoroughly clean and dry contaminated clothing before reuse. Destroy
    contaminated shoes.

   Eye Contact: Immediately flush eyes, including under the eyelids with copious amounts of water for at least
    15 minutes. Seek immediate medical attention.

    Ingestion: Contact a poison control center immediately for instructions. Do not induce vomiting. Give water to
     rinse out mouth. Never give liquids to a person with reduced awareness or becoming unconscious.  If vomiting
    occurs, keep head lower than hips to prevent aspiration.  If not breathing, give artificial respiration by qualified
    personnel. Seek immediate medical attention.

Most Important Symptoms/Effects, Acute and Delayed: Acid burns to skin, eyes, and lungs.

Indication of any immediate medical attention and special treatment needed, if necessary:  If any of the above
symptoms are present, seek immediate medical attention.

 5. FIRE FIGHTING MEASURES

Fire and Explosion Hazards:  Negligible fire hazard.  See Section 9, “Physical and Chemical Properties” for
flammability properties.

Extinguishing Media:
     Suitable: Use extinguishing media appropriate to the surrounding fire.
    Unsuitable: None listed.

Specific Hazards Arising from the Chemical: Thermal decomposition will form oxides of nitrogen and samarium.

Special Protective Equipment and Precautions for Fire-Fighters: Avoid inhalation of material or combustion
byproducts. Wear full protective clothing and NIOSH approved self-contained breathing apparatus (SCBA).
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NFPA Ratings (0 = Minimal; 1 = Slight; 2 = Moderate; 3 = Serious; 4 = Severe)

    Health = 3            Fire = 0          Reactivity = 0

 6. ACCIDENTAL RELEASE MEASURES

Personal Precautions, Protective Equipment and Emergency Procedures:  Immediately contact emergency
personnel. Keep unnecessary personnel away. Use suitable protective equipment; see Section 8, “Exposure Controls
and Personal Protection”.

Methods and Materials for Containment and Clean up: Do not touch spilled material. Notify safety personnel
of spills. Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for
disposal. Isolate hazard area and deny entry.

 7. HANDLING AND STORAGE

Safe Handling Precautions: See Section 8, “Exposure Controls and Personal Protection”. Handle glass ampoules
with care.

Storage:   Store and handle in accordance with  all current regulations and standards.  Keep separated from
incompatible substances (See Section 10, “Stability and Reactivity”).

 8. EXPOSURE CONTROLS AND PERSONAL PROTECTION

Exposure Limits:

  Component: Nitric acid
   NIOSH (REL):     5 mg/m3 (2 ppm; TWA)
                    10 mg/m3 (4 ppm; STEL)
                    65 mg/m3(25 ppm; IDLH)
   ACGIH (TLV):    5 mg/m3 (2 ppm; TWA)
                    10 mg/m3 (4 ppm; STEL)
   OSHA (PEL):      5 mg/m3 (2 ppm; TWA)
  Component: Samarium nitrate
    Exposure Limits not established.

Engineering Controls:  Provide local exhaust or process enclosure ventilation system. Ensure compliance with
applicable exposure limits.

Personal Protection: In accordance with OSHA 29 CFR 1910.132, subpart I, wear appropriate Personal Protective
Equipment (PPE) to minimize exposure to this material.

    Respiratory Protection:    If workplace conditions warrant a respirator, a respiratory protection program that
    meets OSHA 29CFR 1910.134 must be followed. Refer to NIOSH 42 CFR 84 for applicable certified respirators.

    Eye/Face Protection: Wear splash resistant safety goggles with a face shield. An eyewash station should be
     readily available near areas of use.

    Skin and Body Protection: Personal protective equipment for the body should be selected based on the task
    being performed and the risks involved and should be approved by a specialist before handling this product.
    Chemical-resistant gloves should be worn at all times when handling chemicals.
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 9. PHYSICAL AND CHEMICAL PROPERTIES

NOTE: The physical and chemical data provided are for the pure components. No physical or chemical data are
available for this solution. The actual behavior of the solution may differ from the individual components.

 Descriptive Properties:                             Nitric acid                Samarium nitrate
                                                  (10 % of this SRM)             (2.0 % of this SRM)

     Appearance                                      colorless to yellow liquid       yellow solid
      (physical state, color, etc.):
     Molecular Formula:                  HNO3                      Sm(NO3)3
    Molar Mass (g/mol):                         63.01                         336.46
    Odor:                                                  irritating odor                   not available
    Odor threshold:                               not available                    not available
    pH:                                     1 (1 M)                         not available
     Evaporation rate:                             not available                    not available
     Melting point/freezing point (ºC):           –42 (–43 ºF)                 78 (172 ºF)
     Relative Density (g/L) as specific gravity       1.5027 at 25 ºC                 not available
      (water = 1):
    Vapor Pressure (mmHg):                     47.9 at 20 ºC                    not available
    Vapor Density (air = 1):                       3.2                             not available
      Viscosity (cP):                                 not available                    not available
      Solubility(ies):                                 miscible with water and ether    not available
     Partition coefficient                           not available                    not available
     (n-octanol/water):

 Thermal Stability Properties:
     Autoignition Temperature (ºC):               not applicable                   not applicable
    Thermal Decomposition (ºC):                 not applicable                   not available
      Initial boiling point and boiling range (ºC):   83 (181 ºF)                     not available
     Explosive Limits, LEL (Volume %):           not applicable                   not available
     Explosive Limits, UEL (Volume %):           not applicable                   not available
     Flash Point (ºC):                              not applicable                   not available
     Flammability (solid, gas):                      not applicable                   not available

 10. STABILITY AND REACTIVITY

Reactivity: Stable at normal temperatures and pressure.

      Stability:   X       Stable              Unstable

Possible Hazardous Reactions: None listed.

Conditions to Avoid: Contact with combustible or incompatible materials.

Incompatible Materials:  Acids, combustible materials, halo carbons, amines, bases, oxidizing materials, metals,
halogens, metal salts, metal oxides, reducing agents, peroxides, metal carbide, and cyanides.

Fire/Explosion Information: See Section 5, “Fire Fighting Measures”.

Hazardous Decomposition: Thermal decomposition will produce oxides of nitrogen and samarium.

Hazardous Polymerization:          Will Occur     X    Will Not Occur

 11. TOXICOLOGICAL INFORMATION

Route of Exposure:    X    Inhalation     X    Skin        X    Ingestion

Symptoms Related to the Physical, Chemical and Toxicological Characteristics: Burning pain and severe skin
corrosion.
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Potential Health Effects (Acute, Chronic and Delayed):

    Inhalation: Inhalation of nitric acid can damage the mucous membranes and upper respiratory tract. Short term
    exposure may cause irritation and inflammation of the upper respiratory tract, coughing, choking, sore throat,
    shortness of breath, headache, dizziness, and nausea. Long term exposure to acid fumes may cause damage to
     teeth, bronchial irritation, chronic cough, bronchial pneumonia, and gastrointestinal disturbances.  No data
     available on inhalation of samarium nitrate.

    Skin Contact:  Nitric acid can cause severe skin burns. Severity of the damage depends on the concentration
    and duration of exposure. Effects of acid burns may be delayed. No data available on samarium nitrate.

   Eye Contact:  Nitric acid can cause severe eye irritation, corneal burns, permanent eye damage, or blindness.
    Severity of the damage depends on the concentration and duration of exposure. No data available on samarium
     nitrate

    Ingestion:  If ingested, nitric acid can cause severe burns and damage to the gastrointestinal tract. No data
     available on inhalation of samarium nitrate, in animal studies, rare earth salts caused ataxia, writhing, slightly
    labored and depressed respiration, arched back, stretching of limbs on walking and lacrimation.

Numerical Measures of Toxicity:

    Acute Toxicity: Not classified.
         Nitric acid, Rat, Inhalation LC50: 130 mg/m3 (4 h)
       Samarium nitrate, Mouse, Oral LD50: 2160 mg/kg

    Skin Corrosion/Irritation: This SRM contains >1 % of nitric acid and it is classified as Category 1B.

    Serious Eye Damage/Irritation: This SRM contains >1 % nitric acid and it is classified as Category 1.

    Respiratory Sensitization: No data available; not classified.

    Skin Sensitization: No data available; not classified.

   Germ Cell Mutagenicity: No data available; not classified.

    Carcinogenicity: Not classified.
        Listed as a Carcinogen/Potential Carcinogen               Yes       X   No
         Nitric acid and samarium nitrate are not listed by NTP, IARC or OSHA as a carcinogen.

    Reproductive Toxicity: Not classified.
         Nitric acid, Rat, Oral TDLo: 21 150 mg/kg (pregnant 1 d to 21 d)
         Nitric acid, Rat, Oral TDLo: 2345 mg/kg (pregnant 18 d)

    Specific Target Organ Toxicity, Single Exposure: No data available; not classified.

    Specific Target Organ Toxicity, Repeated Exposure: No data available; not classified.

    Aspiration Hazard: No data available.

 12. ECOLOGICAL INFORMATION

Ecotoxicity Data:

    Nitric acid: Starfish (Asterias rubens) LC50: 100 mg/L to 300 mg/L (48 h, renewal/aerated water)
   Samarium nitrate:  No data available.

Persistence and Degradability: No data available.

Bioaccumulative Potential: No data available.

Mobility in Soil: No data available.

Other Adverse effects: No data available.

 13. DISPOSAL CONSIDERATIONS

Waste Disposal: Dispose of waste in accordance with all applicable federal, state, and local regulations. Nitric acid
and samarium nitrate are subject to disposal regulations: U.S. EPA 40 CFR 262, Hazardous Waste Numbers: D002.

 14. TRANSPORTATION INFORMATION

U.S. DOT and IATA: UN1760, Corrosive liquid, n.o.s. (contains nitric acid), Hazard Class 8, Packing Group II,
Excepted Quantities E2.
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 15. REGULATORY INFORMATION

U.S. Regulations:

  CERCLA Sections 102a/103 (40 CFR 302.4):  Nitric acid, 1000 lbs (454 kg) RQ

  SARA Title III Section 302 (40 CFR 355.30):  Nitric acid, 1000 lbs (454 kg) TPQ

  SARA Title III Section 304 (40 CFR 355.40):  Nitric acid, 1000 lbs (454 kg) EPCRA RQ

  SARA Title III Section 313 (40 CFR 372.65):  Nitric acid, 1 % de minimis concentration.

  OSHA Process Safety (29 CFR 1910.119):     Regulated for nitric acid at higher concentrations
                                           500 lbs TQ (≥94.5 % by weight).

  SARA Title III Sections 311/312 Hazardous Categories (40 CFR 370.21):

     ACUTE HEALTH:         Yes.
      CHRONIC HEALTH:     No.
       FIRE:                   No.
      REACTIVE:             No.
      PRESSURE:             No.

State Regulations:
    California Proposition 65: Not listed.

U.S. TSCA Inventory: Nitric acid and samarium nitrate are listed.

TSCA 12(b), Export Notification: Not listed.

Canadian Regulations:
   WHMIS Information: Not provided for this material.
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 16. OTHER INFORMATION

Issue Date: 04 April 2016

Sources:   ChemAdvisor, Inc., SDS Nitric Acid, 22 September 2015.

           ChemAdvisor, Inc., SDS Samarium Trinitrate Hexahydrate, 09 December 2015.

         CDC; NIOSH; NIOSH Pocket Guide to Chemical Hazards; Department of Health and Human
             Services (DHHS), Centers for Disease Control and Prevention (CDC), National Institute for Safety and
             Health;  Nitric Acid, 13 February 2015;  available  at  http://www.cdc.gov/niosh/npg/npgd0447.html
             (accessed Apr 2016).

           Hazardous Substances Data Bank (HSDB), National Library of Medicine's TOXNET system, Nitric Acid
         CAS No. 7697-37-2; available at http://toxnet.nlm.nih.gov/ (accessed Apr 2016).

          ChemIDPlus (HSDB),  National  Library  of  Medicine's TOXNET  system,  Samarium  Nitrate,
         CAS No. 10361-83-8; available at http://toxnet.nlm.nih.gov/ (accessed Apr 2016).





Key of Acronyms:



 ACGIH       American Conference of Governmental Industrial    NRC          Nuclear Regulatory Commission
                 Hygienists
 ALI          Annual Limit on Intake                     NTP           National Toxicology Program
 CAS         Chemical Abstracts Service                 OSHA         Occupational Safety and Health Administration
 CERCLA     Comprehensive Environmental Response,         PEL           Permissible Exposure Limit
               Compensation, and Liability Act
 CFR         Code of Federal Regulations                RCRA        Resource Conservation and Recovery Act
 DOT         Department of Transportation                REL         Recommended Exposure Limit
 EC50          Effective Concentration, 50 %             RM           Reference Material
 EINECS      European Inventory of Existing Commercial       RQ            Reportable Quantity
               Chemical Substances
 EPCRA      Emergency Planning and Community Right-to-Know  RTECS        Registry of Toxic Effects of Chemical Substances
               Act
 IARC          International Agency for Research on Cancer      SARA        Superfund Amendments and Reauthorization Act
 IATA          International Air Transport Association          SCBA         Self-Contained Breathing Apparatus
 IDLH         Immediately Dangerous to Life and Health       SRM          Standard Reference Material
 LC50          Lethal Concentration, 50 %                   STEL          Short Term Exposure Limit
 LD50          Lethal Dose, 50 %                       TLV          Threshold Limit Value
 LEL         Lower Explosive Limit                     TPQ          Threshold Planning Quantity
 MSDS         Material Safety Data Sheet                  TSCA         Toxic Substances Control Act
 NFPA         National Fire Protection Association          TWA        Time Weighted Average
 NIOSH        National Institute for Occupational Safety and Health  UEL         Upper Explosive Limit
 NIST          National Institute of Standards and Technology     WHMIS      Workplace Hazardous Materials Information System
  n.o.s.         Not Otherwise Specified





Disclaimer:  Physical and chemical data contained in  this SDS are provided only for use in assessing the
hazardous nature of the material. The SDS was prepared carefully, using current references; however, NIST does not
certify the data in the SDS.  The certified values for this material are given in the NIST Certificate of Analysis.

Users of this SRM should ensure that the SDS in their possession is current. This can be accomplished by contacting
the SRM Program: telephone (301) 975-2200; fax (301) 948-3730; e-mail srmmsds@nist.gov; or via the Internet at
http://www.nist.gov/srm.
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