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 SECTION 1     PRODUCT AND COMPANY INFORMATION

PRODUCT NAME:   Praseodymium (III) bromide, hydrate

PRODUCT NUMBER:  2959

CAS NUMBER:        225505-12-4

SYNONYMS:         Praseodymium tribromide hydrate

MANUFACTURER:


Prochem, Inc.                                         PHONE:        815-398-1788
826 Roosevelt Road                                          FAX:           815-398-1810
Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                   IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION


CLASSIFICATION OF SUBSTANCE OR MIXTURE



Pictogram


Signal Word         Warning

Hazard Statements

H315               Causes skin irritation.
H319               Causes serious eye irritation.

Precautionary Phrases

P261                 Avoid breathing dust/fume/gas/mist/vapours/spray.
P264             Wash skin thoroughly after handling.
P280              Wear protective gloves/protective clothing/eye protection/face protection/
P305+P351+P338      IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to
                       do. Continue rinsing.

HMIS CLASSIFICATION:
Health: 2            Chronic: *             Flammability: 0                      Reactivity: 0
NFPA RATING:
Health: 2              Fire: 0                  Reactivity Hazard: 0

EYE CONTACT: Dust causes irritation of they eyes.
SKIN CONTACT: Causes irritation of the skin.
INHALATION: Inhalation of dust can lead to irritation of the respiratory tract.
INGESTION: May be harmful if swallowed.
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SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

Formula: PrBr3 � xH2O

Molecular Weight: 380.63 (anhy.)


CHEMICAL NAME                           CAS#              %              ACGIH (TWA)            OSHA (PEL)


Praseodymium (III) bromide                          225505-12-4                  100               No data                  No data

SECTION 4   FIRST AID MEASURES

EYE EXPOSURE: Immediately flush the eyes with copious amounts of water (lukewarm if possible) for several minutes. Assure
flushing under eyelids. A victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if
irritation or redness persists.
INHALATION: Remove victim to fresh air. Closely monitor the victim for signs of respiratory problems, such as difficulty in
breathing, coughing, wheezing, or pain. In such cases, seek immediate medical assistance.
INGESTION: Never give anything by mouth to an unconscious person. Rinse mouth with water. Consult a physician.

SECTION 5   FIREFIGHTING MEASURES

FLASH POINT: Not applicable
AUTO IGNITION TEMPERATURE: Not applicable
EXPLOSION LIMITS: Not applicable
EXTINGUISHING MEDIUM: Water spray, Carbon dioxide, or extinguishing powder.
SPECIAL FIRE FIGHTING PROCEDURES: If involved in a fire, fire fighters should be equipped with a NIOSH approved
positive self-contained breathing apparatus, flame and chemical resistant clothing, hats, boots, and gloves.
HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Hydrogen Bromide gas

SECTION 6   ACCIDENTAL RELEASE MEASURES

PERSONAL PRECAUTIONS: Use personal protective equipment. Keep unprotected persons away. Ensure adequate ventilation.
ENVIRONMENTAL PRECAUTIONS: Do not let product enter drains or be released into the environment.
METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: In case of spill, sweep up and place in a well-marked
container for disposal. Avoid raising dust. Ventilate area and wash spill site after material pickup is complete.

SECTION 7   HANDLING AND STORAGE

PRECAUTIONS FOR SAFE HANDLING: Avoid contact with skin and eyes. Avoid formation of dust. Ensure adequate exhaust
ventilation.
CONDITIONS FOR SAFE STORAGE: Keep in a tightly sealed container. Hygroscopic. Picks up moisture readily from atmosphere.
Handle and store under argon. Store in a cool, dry place in tightly sealed container.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

EYE PROTECTION: Always wear approved safety glasses with side shields, safety goggles, or face shield when handling a chemical
substance in the laboratory.
SKIN PROTECTION: Chemical resistant gloves.
VENTILATION: Handle in an efficient chemical fume hood.
RESPIRATOR:  If in form of fine dust and ventilation is not available a respirator should be worn. The use of respirators requires a
Respirator Protection Program to be in compliance with 29 CFR 19-10.134.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

COLOR AND FORM: Green solid
MOLECULAR WEIGHT: 380.63 (anhy.)
BOILING POINT: 1547° C
MELTING POINT: 691° C
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 SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES (Cont.)

  SPECIFIC GRAVITY: No data available
  VAPOR PRESSURE: Not applicable
  SOLUBILITY: Slightly soluble

 SECTION 10  STABILITY AND REACTIVITY


  STABILITY: Stable
  HAZARDOUS POLYMERIZATION: Will not occur
  CONDITIONS TO AVOID: Moisture
  INCOMPATIBILITY: Strong oxidizing agents
  DECOMPOSITION PRODUCTS: Hydrogen bromide gas and Praseodymium oxide.


 SECTION 11 TOXICOLOGICAL DATA


  CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified as a confirmed
  carcinogen by IARC, ACGIH, NTP, and OSHA.
  MUTAGENIC EFFECTS: No data
  TETRATOGENIC EFFECTS: No data

  To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

 SECTION 12  ECOLOGICAL DATA

  Do not allow product to reach ground water, water bodies, or sewage systems. Do not allow material to be released to the
  environment without proper governmental permits.

 SECTION 13  DISPOSAL CONSIDERATIONS

  Dispose of in according to local, state, and federal regulations.

 SECTION 14  TRANSPORTATION DATA

  Non-hazardous material


 SECTION 15  REGULATORY INFORMATION

  SARA 313 COMPONENTS: This material does not contain any chemical components with know CAS numbers that exceed the
   threshold (De Minimis) reporting levels established by SARA Title III, Section 313.

  SARA 302 COMPONENTS: No chemicals in this material are subject to the reporting requirements of SARA Title III, Section 302.

  SARA 311/312 HAZARDS: Acute Health Hazard

  MASSACHUSETTS RIGHT TO KNOW COMPONENTS: No components are subject to the Massachusetts Right To Know Act.

  PENNSYLVANIA RIGHT TO KNOW COMPONENTS: Praseodymium tribromide

  NEW JERSEY RIGHT TO KNOW COMPONENTS: Praseodymium tribromide

  CALIFORNIA PROP. 65 COMPONENTS: This product does not contain any chemicals known to State of California to cause cancer,
   birth defects, or any other reproductive harm.
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SECTION 16  OTHER INFORMATION


DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
product based on the information.
DATE PREPARED: 04/14
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