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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Ytterbium (III) Nitrate Pentahydrate

 PRODUCT NUMBER:  3806

 CAS NUMBER:        35725-34-9

 MANUFACTURER:


 Prochem, Inc.                                         PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                    IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION

 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Danger

 Hazard Statements

 H272             May intensify fire; oxidizer.
 H315               Causes skin irritation.
 H319               Causes serious eye irritation.
 H335             May cause respiratory irritation.

 Precautionary Phrases

 P210              Keep away from heat/sparks/open flames/hot surfaces.
 P220                 Keep/store away from clothing/combustible material.
 P221               Take any precaution to avoid mixing with combustibles.
 P261                 Avoid breathing dust/fume/gas/mist/vapors/spray.
 P264             Wash skin thoroughly after handling.
 P271              Use only outdoors or in a well-ventilated area.
 P280              Wear protective gloves/protective clothing/eye protection/face protection.
 P302+P352            IF ON SKIN: Wash with plenty of soap and water.
 P304+P340            IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.
 P305+P351+P338      IF IN EYES: Rinse cautiously with waster for several minutes. Remove contact lenses if present and easy to
                        do. Continue rinsing.
 P362               Take off contaminated clothing and wash before reuse.
 P370+P378             In case of fire: Use dry sand, dry chemical or alcohol-resistant foam for extinction.
 P403+P233           Store in a well-ventilated place.
 P422                 Store contents under inert gas.
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)

 HMIS CLASSIFICATION:
 Health: 0              Fire: 0                  Reactivity Hazard: 2
 NFPA RATING:
 Health: 0            Flammability: 0         Reactivity Hazard: 2       Specific Hazard: OX

 EYE CONTACT: May cause slight to mild irritation of the eyes.
 SKIN CONTACT: May cause slight to mild irritation of the skin.
 INHALATION: May be irritating to the nose, mucous membranes, and respiratory tract.
 INGESTION: May be harmful if swallowed.


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Yb(NO3)3 � 5H2O

 Molecular Weight: 449.13


 CHEMICAL NAME                                           CAS#                               %


 Ytterbium (III) Nitrate Pentahydrate                                         35725-34-9                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under
 eyelids. A victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if
 irritation persists.
 INHALATION: Remove to fresh air and keep at rest.  If breathing is difficult, give oxygen.  If not breathing, give artificial
 respiration. Get medical attention if necessary.
 INGESTION: Seek medical assistance immediately. Keep the victim calm. Give the victim water (only if conscious). Induce
 vomiting only if directed by medical personnel.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Not available
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use water spray, alcohol-resistant foam, dry chemical, or carbon dioxide.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Ytterbium oxides and nitrogen oxides

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation. Avoid dust
 formation. Avoid breathing dust.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Small spills can be mixed with vermiculite or sodium
 carbonate and swept up.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Use with adequate ventilation. Avoid
 formation of dust. Keep away from heat and sources of ignition. Avoid contact with skin and eyes.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Keep away from heat and direct sunlight.
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SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EXPOSURE CONTROLS: This product contains no substances occupational exposure limit values.
 EYE PROTECTION: Wear chemical safety glasses or goggles.
 SKIN PROTECTION: Wear nitrile or rubber gloves, apron, or lab coat.
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator.
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES


 COLOR AND FORM: White solid
 ODOR: None
 MOLECULAR WEIGHT: 359.07
 BOILING POINT: Not available
 MELTING POINT: Not available
 SPECIFIC GRAVITY: Not available
 VAPOR DENSITY: No data available
 SOLUBILITY: Very soluble

SECTION 10  STABILITY AND REACTIVITY


 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Contact with strong reducing agents or organic matter. Some nitrate can explode heated to high
 temperatures.
 INCOMPATIBILITY: Flammable substances, reducing agents, water/moisture, organic material, and metal powders
 DECOMPOSITION PRODUCTS: Nitrogen oxides and ytterbium oxides


SECTION 11 TOXICOLOGICAL DATA


 ACUTE TOXICITY: Not available
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No data available.

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 UN1477

 Nitrates, inorganic, n.o.s.

 (Ytterbium (III) nitrate)

 CLASS 5.1

 PG II


 Marine Pollutant: No

 .
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SECTION 15  REGULATORY INFORMATION

 TSCA: Not listed in the TSCA inventory

 SARA 302/304: Not Listed

 SARA 311/312: Reactivity

 SARA (TITLE 313): Not Listed

 PENNSYLVANIA RIGHT TO KNOW: Ytterbium nitrate pentahydrate

 NEW JERSEY RIGHT TO KNOW: Ytterbium nitrate pentahydrate

 CALIFORNIA PROP. 65: Not Listed

 WHMIS CANADA: Class C: Oxidizing material. Class D-2B: Toxic material causing other toxic effects.


SECTION 16  OTHER INFORMATION

 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREPARED: 09/14
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