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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Cerium (IV) Sulfate Hydrate

 PRODUCT NUMBER:  1425-5

 CAS NUMBER:        95838-16-7

 SYNONYMS:          Ceric sulfate hydrate

 MANUFACTURER:

 ProChem, Inc.                                         PHONE:       815-398-1788
 826 Roosevelt Road                                     TOLL FREE:    800-795-8788
 Rockford, IL  61109

                   IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION

 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram

 Signal Word       D
                  Danger
 Hazard Statements

 H303               May be harmful if swallowed
 H314                 Causes severe skin burns and eye damage.
 H335               May cause respiratory irritation
 H410                   Very toxic to aquatic life with long lasting effects.

 Precautionary Phrases

 P260               Do not breathe dusts or mists.
 P264                Wash skin thoroughly after handling.
 P273                    Avoid release to the environment.
 P301+P330+P331         IF SWALLOWED: Rinse mouth. Do NOT induce vomiting.
 P303+P361+P353+P310   IF ON SKIN (or hair): Take off immediately all contaminated clothing. Rinse skin with water/shower.
 P304+P340+P310         IF INHALED: Remove person to fresh air and keep comfortable for breathing. Immediately call a POISON
                        CETNER/doctor.
 P305+P351+P338+P310   IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy
                              to do. Continue rinsing. Immediately call a POISON CENTER/doctor.
 P363                Wash contaminated clothing before reuse.
 P501                   Dispose of contents/container to an approved waste disposal plant.

 HMIS CLASSIFICATION:
 Health: 2              Fire: 0                  Reactivity Hazard: 0
 NFPA RATING:
 Health: 2            Flammability: 0         Reactivity Hazard: 0
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)

 EYE CONTACT: Causes serious eye damage.
 SKIN CONTACT: Causes severe burns to skin.
 INHALATION:  Irritating to the mucous membranes and upper respiratory tract.
 INGESTION: Immediate medical attention is required. Do not induce vomiting. Drink plenty of water.


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Ce(SO4)!XH2O

 Molecular Weight: 332.24 (anhy.)


 CHEMICAL NAME                                           CAS#                               %


 Cerium (IV) Sulfate Hydrate                                                95838-16-7                                                    99.9

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under
 eyelids. A victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Immediately wash affected area thoroughly with soap and water. Remove contaminated clothes if
 necessary. Seek medical assistance if irritation persists.
 INHALATION: Remove to fresh air and keep at rest. Closely monitor the victim for signs of respiratory problems, such as
 difficulty in breathing, coughing, wheezing, or pain. In such cases, seek immediate medical assistance.
 INGESTION: Do not induce vomiting. Give 2-4 cups of milk or water provided person is conscious and alert. Seek medical
 assistance immediately.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Not available
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use Carbon dioxide fire extinguisher. (Powder or Foam) as Water is ineffective. Any dry chemical, dry
 sand measures that are appropriate to local circumstances and the surrounding environment.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Sulfur oxides and cerium oxides

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all required personal protective equipment when using this material. Ensure adequate ventilation
 and use ventilation hood. Avoid the formation of dust. Avoid breathing vapors, mist, gas, or dust.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Pick up and arrange disposal without creating dust. Sweep
 up and keep in suitable, closed containers for disposal.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Use with adequate ventilation. Avoid
 contact with skin and eyes. Avoid formation of dust.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield.
 SKIN PROTECTION: Wear nitrile or rubber gloves, apron, or lab coat.
 VENTILATION: Provide local exhaust, preferably mechanical.
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SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION (Cont.)

 RESPIRATOR: Use an approved respirator.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

 COLOR AND FORM: White to off white solid
 ODOR: None
 MOLECULAR WEIGHT: 332.24 (anhy.)
 BOILING POINT: No data available
 MELTING POINT: 200° C (dec.).
 SPECIFIC GRAVITY: 3.24.
 VAPOR DENSITY: No data available
 SOLUBILITY IN WATER: Soluble in small amounts. Hydrolyzes in large amounts of water.

SECTION 10  STABILITY AND REACTIVITY

 STABILITY: Stable. Moisture sensitive.
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: No data available
 INCOMPATIBILITY: No data available.
 DECOMPOSITION PRODUCTS: Sulfur oxides and cerium oxides


SECTION 11 TOXICOLOGICAL DATA

 ACUTE TOXICITY: Not available
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available
 RTECS: Not available

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 TOXICITY TO DAPHNIA AND OTHER AQUATIC INVERTEBRATES: Static test EC50 – Daphnia magna (water flea) – 1.9 mg/l – 48h
 TOXICITY TO ALGAE: Static test ErC50 – Pseudokirchneriella subcapitata (green algea) – 0.658 mg/l – 72h. Static test NOEC-
                        Pseudokirchneriella subcapitata (green algae) – 0.555 mg/l – 72h.


 Very toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.
 This product contains substances which are hazardous for the environment and will cause long-term effects.
 Do not allow material to contaminate ground water system.

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 UN3260.
 Corrosive solid, acidic, inorganic, n.o.s.
 Class 8


 PG II
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SECTION 15  REGULATORY INFORMATION

 TSCA – Listed – Toxic Substance Control Act, (40 CFR Part 710)
 SARA 302: Not listed
 SARA (TITLE 313): Not listed -
 SARA 311/312: Acute Health Hazard
 MASSACHUSETTS RIGHT TO KNOW: No components are subject to the Massachusetts Right to Know Act.


SECTION 16  OTHER INFORMATION

 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, ProChem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREVIOUSLY REVISED: 03/22
 REVISED DATE: 08/26
 REVISED SUMMARY: removed fax number. Updated section 2, section 15. All other details in this document about this product
 remained unchanged. Updates made by EHS 08/10/206

 EHS/SDS DEPT.
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