Yttrium (III) Sulfide 3871 SDS
Publisher: ProChem, Inc.
Source: https://resds.com/document/yttrium-iii-sulfide-sds-prochem-en-bb6aa8fc1b
Text extracted from the original PDF. Tables, symbols and OCR may differ. Check the original PDF for safety-critical details.
Page 1
 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Yttrium (III) Sulfide

 PRODUCT NUMBER:  3871

 CAS NUMBER:        12039-19-9

 MANUFACTURER:


 Prochem, Inc.                                         PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                    IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION

 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Danger

 Hazard Statements

 H261                    In contact with water releases flammable gas.
 H315               Causes skin irritation.
 H319               Causes serious eye irritation.
 H335             May cause respiratory irritation.

 Precautionary Phrases

 P231+P232          Handle under inert gas. Protect from moisture.
 P261                 Avoid breathing dust/fume/gas/mist/vapors/spray.
 P280              Wear protective gloves/protective clothing/eye protection/face protection.
 P305+P351+P338      IF IN EYES: Rinse cautiously with waster for several minutes. Remove contact lenses if present and easy to
                        do. Continue rinsing.

 HMIS CLASSIFICATION:
 Health: 2              Fire: 1                  Reactivity Hazard: 1
 NFPA RATING:
 Health: 2            Flammability: 1         Reactivity Hazard: 1

 EYE CONTACT: Causes serious eye irritation.
 SKIN CONTACT: Causes skin irritation.
 INHALATION: May cause respiratory tract irritation.
 INGESTION: Gastric juices my cause released of toxic hydrogen sulfide.
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SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Y2S3

 Molecular 273.93


 CHEMICAL NAME                                           CAS#                               %


 Yttrium (III) Sulfide                                                       12039-19-9                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under
 eyelids. A victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if
 irritation persists.
 INHALATION: Remove to fresh air and keep at rest.  If breathing is difficult, give oxygen.  If not breathing, give artificial
 respiration. Get medical attention.
 INGESTION: Seek medical assistance immediately. Keep the victim calm. Give the victim water (only if conscious). Induce
 vomiting only if directed by medical personnel.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Not available
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use carbon dioxide or dioxide. Do NOT use water. Contact with water liberates extremely flammable
 gases.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Hydrogen sulfide, sulfur oxides, and yttrium oxides.

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation. Avoid the
 formation of dust. Avoid breathing vapors, mist, gas, or dust. Keep away from sources of ignition
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Cover spill with dry sodium carbonate or dolomite. Sweep
 up and place in suitable container for proper disposal.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Avoid contact with skin and eyes. Use with
 adequate ventilation. Avoid formation of dusts and aerosols.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Store away from water/moisture.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EXPOSURE CONTROLS:
 Component                 Exposure Limits              Basis                           Entity
 Yttrium                      1 mg/m3                   TLV                     ACGIH
                             1 mg/m3                  PEL                   OSHA
 TLV: Threshold Limit Value over 8 hours of work.            PEL: Permissible Exposure Limit

 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield.
 SKIN PROTECTION: Wear nitrile or rubber gloves, and a complete suit protecting against chemicals.
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator.
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.
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SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

 COLOR AND FORM: Yellow powder
 ODOR: Like rotten eggs
 MOLECULAR WEIGHT: 273.93
 BOILING POINT: No data available
 MELTING POINT: No data available
 SPECIFIC GRAVITY: No data available
 SOLUBILITY: Insoluble

SECTION 10  STABILITY AND REACTIVITY

 STABILITY: In contact with water releases flammable gases which may ignite spontaneously
 HAZARDOUS POLYMERIZATION: Reacts with water and acids.
 CONDITIONS TO AVOID: Contact of dust cloud with an ignition source. Contact with water liberates extremely flammable gases.
 INCOMPATIBILITY: Active metals, mineral acids, oxidizing agents, water, and moisture.
 DECOMPOSITION PRODUCTS: Hydrogen sulfide, sulfur oxides, and yttrium oxides.


SECTION 11 TOXICOLOGICAL DATA


 ACUTE TOXICITY: Not available
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available
 CHRONIC TOXICITY: Not available
 RTECS: No data

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No information available

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 UN3134

 Water-reactive solid, toxic, n.o.s.

 (Yttrium (III) sulfide)

 CLASS 4.3 (6.1)

 PG II


 Marine Pollutant: No


SECTION 15  REGULATORY INFORMATION

 TSCA: Listed in the TSCA inventory

 SARA 302/304: Not Listed

 SARA 311/312: Not Listed

 SARA (TITLE 313): Not Listed

 CALIFORNIA PROP. 65: Not Listed
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SECTION 16  OTHER INFORMATION


 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREPARED: 05/15
 SDS DEPT.
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