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 ALFAA47240

       Cerium(IV) oxide, 20% in H2O, nanoparticle dispersion, high pH

   SECTION 1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING


产品说明:产品说明:产品说明:产品说明:                氧化铈(IV)氧化铈(IV)氧化铈(IV)氧化铈(IV),,,,20%20%20%20% ininininH_2OH_2OH_2OH_2O
Product Description:               Cerium(IV) oxide, 20% in H2O, nanoparticle dispersion, high pH

Cat No. :                        47240
Molecular Formula             CeO2

Supplier                         Avocado Research Chemicals Ltd.
                                        (Part of Thermo Fisher Scientific)
                                 Shore Road, Heysham
                                     Lancashire, LA3 2XY,
                                    United Kingdom
                                        Office Tel: +44 (0) 1524 850506
                                        Office Fax: +44 (0) 1524 850608


Emergency Telephone Number     For information US call: 001-800-227-6701 / Europe call: +32 14 57 52 11
                               Emergency Number US:001-201-796-7100 / Europe: +32 14 57 52 99
                         CHEMTREC Tel. No. US:001-800-424-9300 / Europe:001-703-527-3887

E-mail address                    begel.sdsdesk@thermofisher.com

Recommended Use                 Laboratory chemicals.
Uses advised against           No Information available

                           SECTION 2. HAZARD IDENTIFICATION


            Physical State                      Appearance                          Odor
                   Liquid                         Red brown                              Odorless

                                        Emergency Overview
       The product contains no substances which at their given concentration are considered to be hazardous to health.


Classification of the substance or mixture
Based on available data, the classification criteria are not met

Label Elements

None required





Physical and Chemical Hazards
None identified.
Health Hazards
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The product contains no substances which at their given concentration are considered to be hazardous to health.
Environmental hazards
Contains no substances known to be hazardous to the environment or not degradable in waste water treatment plants. Is not likely
mobile in the environment due its low water solubility. Spillage unlikely to penetrate soil. The product is insoluble and sinks in
water.

This product does not contain any known or suspected endocrine disruptors.

                  SECTION 3. COMPOSITION/INFORMATION ON INGREDIENTS


                           Component                              CAS No                Weight %
                                  Water                                            7732-18-5                  80
                               Cerium oxide                                         1306-38-3                  20



                            SECTION 4. FIRST AID MEASURES


General Advice
Show this safety data sheet to the doctor in attendance. Immediate medical attention is required.

Eye Contact
Rinse immediately with plenty of water, also under the eyelids, for at least 15 minutes. Get medical attention.

Skin Contact
Wash off immediately with plenty of water for at least 15 minutes. Get medical attention immediately if symptoms occur.

Inhalation
Remove to fresh air. Get medical attention immediately if symptoms occur.

Ingestion
Clean mouth with water and drink afterwards plenty of water. Get medical attention if symptoms occur.

Most important symptoms and effects
None reasonably foreseeable. Inhalation of high vapor concentrations may cause symptoms like headache, dizziness, tiredness,
nausea and vomiting: Product is a corrosive material. Use of gastric lavage or emesis is contraindicated. Possible perforation of
stomach or esophagus should be investigated: Ingestion causes severe swelling, severe damage to the delicate tissue and danger
of perforation


Self-Protection of the First Aider
No special precautions required.

Notes to Physician
Treat symptomatically. Symptoms may be delayed.

                          SECTION 5. FIRE-FIGHTING MEASURES


Suitable Extinguishing Media
Carbon dioxide (CO 2). Powder. Water spray. In case of major fire and large quantities: Evacuate area. Fight fire remotely due to
the risk of explosion. CO 2, dry chemical, dry sand, alcohol-resistant foam. Water mist may be used to cool closed containers.

Extinguishing media which must not be used for safety reasons
Water.

Specific Hazards Arising from the Chemical
Thermal decomposition can lead to release of irritating gases and vapors. The product causes burns of eyes, skin and mucous
membranes. Reacts violently with water. Flammable. Containers may explode when heated. Vapors may form explosive mixtures
with air. Vapors may travel to source of ignition and flash back.


Protective Equipment and Precautions for Firefighters
______________________________________________________________________________________________
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As in any fire, wear self-contained breathing apparatus pressure-demand, MSHA/NIOSH (approved or equivalent) and full
protective gear.

                       SECTION 6. ACCIDENTAL RELEASE MEASURES


Personal Precautions
Ensure adequate ventilation. Use personal protective equipment as required.


Environmental Precautions
Should not be released into the environment. Do not allow material to contaminate ground water system. Do not flush into surface
water or sanitary sewer system.


Methods for Containment and Clean Up
Sweep up and shovel into suitable containers for disposal.


Refer to protective measures listed in Sections 8 and 13.

                          SECTION 7. HANDLING AND STORAGE


Handling
Wear personal protective equipment/face protection. Ensure adequate ventilation. Avoid contact with skin, eyes or clothing. Avoid
ingestion and inhalation.

Storage
Corrosives area. Keep away from water or moist air. Keep containers tightly closed in a dry, cool and well-ventilated place.
Containers should be dated when opened and tested periodically for the presence of peroxides. Should crystals form in a
peroxidizable liquid, peroxidation may have occurred and the product should be considered extremely dangerous. In this instance,
the container should only be opened remotely by professionals. Keep away from heat, sparks and flame.

Specific Use(s)
Use in laboratories

                  SECTION 8. EXPOSURE CONTROLS/PERSONAL PROTECTION

Control Parameters



Legend

ACGIH - American Conference of Governmental Industrial Hygienists
OSHA - Occupational Safety and Health Administration
NIOSH: NIOSH - National Institute for Occupational Safety and Health

Monitoring methods
BS EN 14042:2003 Title Identifier: Workplace atmospheres. Guide for the application and use of procedures for the assessment of
exposure to chemical and biological agents. MDHS70 General methods for sampling airborne gases and vapours MDHS 88
Volatile organic compounds in air. Laboratory method using diffusive samplers, solvent desorption and gas chromatography MDHS
96 Volatile organic compounds in air - Laboratory method using pumped solid sorbent tubes, solvent desorption and gas
chromatography MDHS 91 Metals and metalloids in workplace air by X-ray fluorescence spectrometry MDHS 99 Metals in air by
ICP-AES

Exposure Controls

Engineering Measures
Ensure that eyewash stations and safety showers are close to the workstation location. Ensure adequate ventilation, especially in
confined areas. Use explosion-proof electrical/ventilating/lighting equipment. Wherever possible, engineering control measures
such as the isolation or enclosure of the process, the introduction of process or equipment changes to minimise release or contact,
and the use of properly designed ventilation systems, should be adopted to control hazardous materials at source.
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Personal protective equipment

   Eye Protection                Goggles (European standard - EN 166)

   Hand Protection                  Protective gloves

    Glove material     Breakthrough time  Glove thickness   EU standard             Glove comments
        Nitrile rubber      See manufacturers               -          EN 374             (minimum requirement)
        Viton (R)        recommendations
      Natural rubber
       Neoprene
       PVC
       Butyl rubber
    Neoprene gloves
Inspect gloves before use.
Please observe the instructions regarding permeability and breakthrough time which are provided by the supplier of the gloves.
(Refer to manufacturer/supplier for information)
Ensure gloves are suitable for the task: Chemical compatability, Dexterity, Operational conditions, User susceptibility, e.g.
sensitisation effects, also take into consideration the specific local conditions under which the product is used, such as the danger
of cuts, abrasion.
Remove gloves with care avoiding skin contamination.

   Skin and body protection       Long sleeved clothing

   Respiratory Protection       When workers are facing concentrations above the exposure limit they must use
                                      appropriate certified respirators.
                              To protect the wearer, respiratory protective equipment must be the correct fit and be used
                               and maintained properly

   Large scale/emergency use    Use a NIOSH/MSHA or European Standard EN 136 approved respirator if exposure limits
                                    are exceeded or if irritation or other symptoms are experienced
                           Recommended Filter type: Organic gases and vapours filter low boiling organic solvent
                               Type AX Brown conforming to EN371 or Type A Brown conforming to EN14387 Particulates
                                                       filter conforming to EN 143

   Small scale/Laboratory use     Use a NIOSH/MSHA or European Standard EN 149:2001 approved respirator if exposure
                                              limits are exceeded or if irritation or other symptoms are experienced.
                           Recommended half mask:- Valve filtering: EN405; or; Half mask: EN140; plus filter, EN
                                    141; Particle filtering: EN149:2001
                           When RPE is used a face piece Fit Test should be conducted


Hygiene Measures                Handle in accordance with good industrial hygiene and safety practice.

Environmental exposure controls   Prevent product from entering drains. Do not allow material to contaminate ground water
                                   system.

                     SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES


Appearance                   Red brown
Physical State                        Liquid

Odor                              Odorless
Odor Threshold               No data available
pH                             8
Melting Point/Range            No data available
Softening Point                No data available
Boiling Point/Range            No information available
Flash Point                   No information available           Method - No information available
Evaporation Rate              No data available
Flammability (solid,gas)            Not applicable                         Liquid
Explosion Limits               No data available
______________________________________________________________________________________________
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Vapor Pressure                No data available
Vapor Density                 No data available                         (Air = 1.0)
Specific Gravity  / Density           1.23 g/cm3            @ 20 °C
Bulk Density                      Not applicable                         Liquid
Water Solubility                     Immiscible
Solubility in other solvents       No information available
Partition Coefficient (n-octanol/water)
Autoignition Temperature        No data available
Decomposition Temperature      No data available
Viscosity                    No data available
Explosive Properties                                               Vapors may form explosive mixtures with air
Oxidizing Properties            No information available


Molecular Formula             CeO2
Molecular Weight                  172.12



                         SECTION 10. STABILITY AND REACTIVITY


Stability                             Stable under normal conditions.

Hazardous Reactions            None under normal processing.
Hazardous Polymerization        No information available.

Conditions to Avoid               Exposure to moist air or water. Exposure to moisture. Keep away from open flames, hot
                                     surfaces and sources of ignition.

Materials to avoid                  Strong bases. Oxidizing agent.


Hazardous Decomposition Products Cerium oxide.

                        SECTION 11. TOXICOLOGICAL INFORMATION


Product Information

(a) acute toxicity;
Toxicology data for the components

           Component                    LD50 Oral                LD50 Dermal             LC50 Inhalation
                Water                                               -                                            -                                            -
             Cerium oxide                 >5000 mg/kg  ( Rat )          >2000 mg/kg  ( Rat )           >5.05 mg/L  ( Rat ) 4 h

(b) skin corrosion/irritation;       No data available


(c) serious eye damage/irritation;   No data available


(d) respiratory or skin sensitization;
   Respiratory                No data available
   Skin                     No data available

(e) germ cell mutagenicity;       No data available

(f) carcinogenicity;             No data available

                                      Limited evidence of a carcinogenic effect The table below indicates whether each agency
                                has listed any ingredient as a carcinogen
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(g) reproductive toxicity;         No data available


(h) STOT-single exposure;        No data available

   Results / Target organs          Central nervous system (CNS)


(i) STOT-repeated exposure;      No data available

   Target Organs              No information available.


(j) aspiration hazard;            No data available

Symptoms  / effects,both acute and Inhalation of high vapor concentrations may cause symptoms like headache, dizziness,
delayed                                tiredness, nausea and vomiting: Product is a corrosive material. Use of gastric lavage or
                                 emesis is contraindicated. Possible perforation of stomach or esophagus should be
                                        investigated: Ingestion causes severe swelling, severe damage to the delicate tissue and
                                  danger of perforation

                         SECTION 12. ECOLOGICAL INFORMATION


Ecotoxicity effects                 Contains a substance which is:. The product contains following substances which are
                                  hazardous for the environment. Toxic to aquatic organisms. May cause long-term adverse
                                         effects in the environment. Do not allow material to contaminate ground water system.


           Component                Freshwater Fish         Water Flea        Freshwater Algae         Microtox
             Cerium oxide             LC50 >100 mg/L/96h   EC50 >100 mg/L/48h
                                           (Brachydanio rerio)


Persistence and Degradability      Product contains heavy metals. Discharge into the environment must be avoided. Special
                                      pre-treatment is necessary
   Persistence                May persist, based on information available, Immiscible with water.
   Degradation in sewage          Contains substances known to be hazardous to the environment or not degradable in waste
   treatment plant                 water treatment plants.


Bioaccumulative Potential        May have some potential to bioaccumulate; Product has a high potential to bioconcentrate



Mobility in soil                        Spillage unlikely to penetrate soil The product is insoluble and sinks in water Is not likely
                                   mobile in the environment due its low water solubility


Endocrine Disruptor Information
Persistent Organic Pollutant        This product does not contain any known or suspected substance
Ozone Depletion Potential           This product does not contain any known or suspected substance

                         SECTION 13. DISPOSAL CONSIDERATIONS


Waste from Residues/Unused      Waste is classified as hazardous. Dispose of in accordance with the European Directives
Products                        on waste and hazardous waste. Dispose of in accordance with local regulations.

Contaminated Packaging           Dispose of this container to hazardous or special waste collection point. Empty containers
                                          retain product residue, (liquid and/or vapor), and can be dangerous. Keep product and
                                empty container away from heat and sources of ignition.

Other Information              Do not flush to sewer. Waste codes should be assigned by the user based on the
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                                        application for which the product was used. Can be landfilled or incinerated, when in
                                  compliance with local regulations. Do not empty into drains. Large amounts will affect pH
                               and harm aquatic organisms.

                         SECTION 14. TRANSPORT INFORMATION


Road and Rail Transport           Not Regulated



IMDG/IMO                        Not regulated



IATA                             Not regulated



Special Precautions for User      No special precautions required

                         SECTION 15. REGULATORY INFORMATION



International Inventories
China, X = listed, Australia, U.S.A. (TSCA), Canada (DSL/NDSL), Europe (EINECS/ELINCS/NLP), Australia (AICS), Korea (KECL), China (IECSC),
Japan (ENCS), Philippines (PICCS).

    Component        The        List of    IECSC   EINECS   TSCA   DSL   PICCS  ENCS    ISHL    AICS    KECL
                     Inventory of dangerous
                   Hazardous  goods GB
                    Chemicals   12268 -
                        (2015      2012
                         Edition)
       Water                    -                 -        X      231-791-2    X      X      X      X             X     KE-35400
    Cerium oxide               -                 -        X      215-150-4    X      X      X      X      X      X     KE-05392



National Regulations


                            SECTION 16. OTHER INFORMATION


Prepared By                         Health, Safety and Environmental Department
Revision Date                     04-Aug-2026
Revision Summary                Not applicable.

Training Advice
Chemical hazard awareness training, incorporating labelling, Safety Data Sheets (SDS), Personal Protective Equipment (PPE) and
hygiene.
Use of personal protective equipment, covering appropriate selection, compatibility, breakthrough thresholds, care, maintenance, fit
and standards.
First aid for chemical exposure, including the use of eye wash and safety showers.
Fire prevention and fighting, identifying hazards and risks, static electricity, explosive atmospheres posed by vapours and dusts.
Chemical incident response training.

                                              Legend

CAS - Chemical Abstracts Service                          TSCA - United States Toxic Substances Control Act Section 8(b)
                                                                       Inventory
EINECS/ELINCS - European Inventory of Existing Commercial Chemical DSL/NDSL - Canadian Domestic Substances List/Non-Domestic
Substances/EU List of Notified Chemical Substances                  Substances List
PICCS - Philippines Inventory of Chemicals and Chemical Substances  ENCS - Japanese Existing and New Chemical Substances
______________________________________________________________________________________________
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IECSC - Chinese Inventory of Existing Chemical Substances          AICS - Australian Inventory of Chemical Substances
KECL - Korean Existing and Evaluated Chemical Substances         NZIoC - New Zealand Inventory of Chemicals


WEL - Workplace Exposure Limit                        TWA - Time Weighted Average
ACGIH - American Conference of Governmental Industrial Hygienists   IARC - International Agency for Research on Cancer
DNEL - Derived No Effect Level                           PNEC - Predicted No Effect Concentration
RPE - Respiratory Protective Equipment                        LD50 - Lethal Dose 50%
LC50 - Lethal Concentration 50%                            EC50 - Effective Concentration 50%
NOEC - No Observed Effect Concentration                 POW - Partition coefficient Octanol:Water
PBT - Persistent, Bioaccumulative, Toxic                       vPvB - very Persistent, very Bioaccumulative


ICAO/IATA - International Civil Aviation Organization/International Air   IMO/IMDG - International Maritime Organization/International Maritime
Transport Association                                          Dangerous Goods Code
ADR - European Agreement Concerning the International Carriage of   MARPOL - International Convention for the Prevention of Pollution from
Dangerous Goods by Road                                         Ships
OECD - Organisation for Economic Co-operation and Development    ATE - Acute Toxicity Estimate
BCF - Bioconcentration factor                           VOC - (Volatile Organic Compound)

Key literature references and sources for data
https://echa.europa.eu/information-on-chemicals
Suppliers safety data sheet, Chemadvisor - LOLI, Merck index, RTECS

Physical hazards              On basis of test data
Health Hazards                       Calculation method
Environmental hazards              Calculation method




                                                    Disclaimer
 The information provided in this Safety Data Sheet is correct to the best of our knowledge, information and belief at the
 date of its publication. The information given is designed only as a guidance for safe handling, use, processing, storage,
   transportation, disposal and release and is not to be considered a warranty or quality specification. The information
relates only to the specific material designated and may not be valid for such material used in combination with any other
                                 materials or in any process, unless specified in the text

                    End of Safety Data Sheet
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