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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Praseodymium (III) Carbonate, Octahydrate

 PRODUCT NUMBER:  2962

 CAS NUMBER:        14948-62-0

 MANUFACTURER:


 Prochem, Inc.                                         PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                    IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION

 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Not a dangerous substance according to GHS.

 HMIS CLASSIFICATION:
 Health: 1              Fire: 0                  Reactivity Hazard: 1
 NFPA RATING:
 Health: 0            Flammability: 0         Reactivity Hazard: 0

 EYE CONTACT: May cause eye irritation.
 SKIN CONTACT: May cause skin irritation.
 INHALATION: May cause irritation to the nose, throat, and respiratory tract.
 INGESTION: May be harmful if swallowed.


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Pr2(CO3)3 � 8H2O

 Molecular Weight: 605.97


 CHEMICAL NAME                                           CAS#                               %


 Praseodymium (II) Carbonate Octahydrate                                  14948-62-0                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water. Assure flushing under eyelids. A victim may need
 assistance in keeping their eyelids open. Get medical attention if redness or irritation persists.
 SKIN EXPOSURE: Wash affected area with soap and water. Remove contaminated clothes if necessary. Seek medical
 assistance if irritation or redness persists.
 INHALATION: Remove to fresh air and keep at rest.  If breathing is difficult, give oxygen.  If not breathing, give artificial
 respiration. Get medical attention if necessary.
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SECTION 4   FIRST AID MEASURES (Cont.)

 INGESTION: Do NOT induce vomiting. Never give anything by mouth to an unconscious person.  If conscious, wash out mouth
 with water. Get medical attention if necessary.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Product is not flammable.
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use fire fighting measures that suit the surrounding fire.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Carbon oxides and praseodymium oxide.

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing it to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Sweep up avoiding raising dust and place in a well-marked
 container for disposal.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Ensure adequate ventilation.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Keep in dry area. Store away from acids. Slightly
 hygroscopic.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EXPOSURE CONTROLS: Contains no substances with occupational exposure limit values.
 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield
 SKIN PROTECTION: Wear nitrile or rubber gloves, and a complete suit protecting against chemicals
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

 COLOR AND FORM: Green solid
 ODOR: None
 MOLECULAR WEIGHT: 605.97
 BOILING POINT: No data available
 MELTING POINT: No data available
 SPECIFIC GRAVITY: No data available
 VAPOR DENSITY: No data available
 SOLUBILITY: Insoluble

SECTION 10  STABILITY AND REACTIVITY


 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Water, humidity, and moisture (slightly hygroscopic)
 INCOMPATIBILITY: Acids
 DECOMPOSITION PRODUCTS: Carbon oxides and praseodymium oxide.
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SECTION 11 TOXICOLOGICAL DATA


 ACUTE TOXICITY: Not available
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No data available.

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 Not a dangerous good.


SECTION 15  REGULATORY INFORMATION

 TSCA: Listed in the TSCA inventory

 DSCL (EEC): Listed on the DSCL inventory

 SARA 302/304: Not Listed

 SARA 311/312: No data available

 SARA (TITLE 313): Not Listed

 CALIFORNIA PROP. 65: Not Listed


SECTION 16  OTHER INFORMATION


 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREPARED: 08/14
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