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SECTION 1     PRODUCT AND COMPANY INFORMATION

PRODUCT NAME:  CERIUM (III) NITRATE SOLUTION

MANUFACTURER:


Prochem, Inc.                                         PHONE:        815-398-1788
826 Roosevelt Road                                          FAX:           815-398-1810
Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                   IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION


CLASSIFICATION OF SUBSTANCE OR MIXTURE



Pictogram



Signal Word    Danger

Hazard Statements

H272             May intensify fire; oxidizer
H332                Harmful if Inhaled.
H302                Harmful if Swallowed
H314               Causes severe skin burns and eye damage

Precautionary Phrases


P210              Keep away from heat/sparks/open flames/hot surfaces. –No smoking
P220                 Keep/Store away from clothing/…/combustible materials.
P261                 Avoid breathing dust/fume/gas/mist/vapous/spray.
P280              Wear protective gloves/eye protection/face protection
P404                 Store in closed container.
P304 + P340           IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.

HMIS CLASSIFICATION:
Health: 3            Flammability: 0                 Physical Hazard: 1

NFPA RATING:
Health: 3              Fire: 0                               Instability: 1

POTENTIAL HEALTH EFFECTS:  Inhalation, Ingestion, Skin and Eye
EYE CONTACT: Causes severe irritation to eyes.
SKIN CONTACT: Causes irritation to skin.
INHALATION: Causes irritation to respiratory system.
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)

INGESTION: No data
ACUTE HEALTH EFFECTS: No data
CHRONIC HEALTH EFFECTS: No information available on long-term chronic effects.

SECTION 3     COMPOSITION / INFORMATION ON INGREDIENTS

Formula:  H2Ce(NO3)6

Molecular Weight: 514.1800


 CHEMICAL NAME                        CAS#              %               ACGIH (TWA)            OSHA (PEL)


Cerium (III) Nitrate                               10294-41-4                       65-75               Not Determined                Not Determined


Nitric Acid                                       7697-37-2                         0-5


Water                                           7732-18-5                        25-35               Not Applicable                 Not Applicable

SECTION 4   FIRST AID MEASURES


EYE EXPOSURE: Immediately flush the eyes with copious amounts of water (lukewarm if possible) for at least 15 minutes.
Assure flushing under eyelids. A victim may need assistance in keeping their eyelids open. Got immediate competent medical
attention.
SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if
irritation, burns, or redness persists.
INHALATION: Remove victim to fresh air. Closely monitor the victim for signs of respiratory problems, such as difficulty in breathing,
coughing, wheezing, or pain. In such cases seek immediate medical assistance. Give oxygen if deemed necessary.  If not breathing
administer CPR. Get emergency care immediately.
INGESTION: Seek medical assistance immediately. Keep the victim calm. Do not induce vomiting.

SECTION 5   FIREFIGHTING MEASURES

EXTINGUISHING MEDIUM: Use water only
SPECIAL FIRE FIGHTING PROCEDURES:   If this product is involved in a fire, fire fighters should be equipped with a NIOSH
approved positive pressure self-contained breathing apparatus and full protective clothing. Use water spray to cool fire-exposed
containers and structures.  .
HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: If involved in a fire this material may emit oxides and
nitrogen.
UNUSUAL FIRE OR EXPLOSION HAZARDS: None known.

SECTION 6   ACCIDENTAL RELEASE MEASURES

PERSONAL PRECUATIONS: Evacuate all personnel to safe areas. Use adequate protection when handling. Use self-contained
breathing apparatus for large spills.
ENVIRONMENTAL PRECAUTIONS: This material should be prevented from contaminating soil or from sewer and drainage systems
and bodies of water.
METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Isolate spillage. Absorb spill with inert materials, then
place in applicable chemical waste container.

SECTION 7   HANDLING AND STORAGE

PRECAUTIONS FOR SAFE HANDLING: Be sure to have appropriate exhaust and ventilation.
CONDITIONS FOR SAFE STORAGE: Keep containers tightly closed. Store in a cool, dry, and well-ventilated area away from heat and
all sources of ignition. Store away from incompatible materials..
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SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

EYE PROTECTION: Always wear approved safety glasses w/side shields, or safety goggles, faceshield when
handling a chemical substance in the laboratory.
SKIN PROTECTION: Wear PVC, rubber, neoprene.

VENTILATION:  If possible, handle the material in a local exhaust hood.
RESPIRATOR:   If ventilation is not available, a high efficiency acid/mist respirator should be worn. The use of respirators required a
Respirator Protection Program to be in compliance with 29CFR 1910.34.
ADDITIONAL PROTECTION: Protection to avoid contact with clothing and shoes.
OTHER PROTECTIVE EQUIPMENT: Eye was and quick-drench shower facilities should be available in work area. Use in a
controlled environment. Do not smoke, eat, or drink in area.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

COLOR AND FORM: Clear to yellow liquid
MELTING POINT: Not applicable
BOILING POINT: No data
FLASH POINT: Not applicable
MOLECULAR  WEIGHT:
ODOR: Acrid, pungent
VAPOR PRESSURE: Not applicable
VAPOR DENSITY (AIR = 1): Not applicable
% VOLATILE BY VOLUME: Non volatile
SOLUBILITY IN WATER: Not applicable

SECTION 10  STABILITY AND REACTIVITY

STABILITY: Stable
HAZARDOUS POLYMERIZATION: Will not occur
CONDITIONS TO AVOID: Excessive temperatures
INCOMPATIBILITY: Reducing agents
DECOMPOSITION PRODUCTS: Gaseous oxides of nitrogen form on decomposition of nitrates by temperature exceeding
150 deg. C. and/or by oxidation reactions.

SECTION 11 TOXICOLOGICAL DATA

CARCINOGENIC EFFECTS: No
MUTAGENIC EFFECTS: No
TETRATOGENIC EFFECTS: No

To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

No information available

SECTION 13  DISPOSAL CONSIDERATIONS

Retain all contaminated solage from removal and treatment. Dispose of in according to local
state and federal regulations.
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SECTION 14  TRANSPORTATION DATA

Nitrates, inorganics, n.o.s.

Class 5.1

UN1477

PGIII


SECTION 15  REGULATORY INFORMATION

TSCA Listed in TSCA inventory
SARA (TITLE 313): Total Nitrates (in solution)
RCRA STATUS: Meets criteria for nitrated and should be managed as a hazardous waste.


SECTION 16  OTHER INFORMATION

DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
product based on the information.
DATE PREPARED: 09/13
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