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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Yttrium (III) Fluoride

 PRODUCT NUMBER:  3850

 CAS NUMBER:        13709-49-4

 SYNONYMS:          Yttrium trifluoride

 MANUFACTURER:

 ProChem, Inc.                                        PHONE:        815-398-1788
 826 Roosevelt Road                                     TOLL FREE:    800-795-8788
 Rockford, IL 61109

                   IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION

 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Warning

 Hazard Statements

 H302+H312+H332    Harmful if swallowed or if in contact with skin, or if inhaled.
 H331                 Toxic if inhaled.
 H315              Causes skin irritation.
 H319              Causes serious eye irritation.
 H335             May cause respiratory irritation.

 Precautionary Phrases

 P261                Avoid breathing dust/fume/gas/mist/vapors/spray.
 P264             Wash skin thoroughly after handling.
 P270             Do not eat, drink, or smoke when using this product.
 P271              Use only outdoors or in a well-ventilated area.
 P280              Wear protective gloves/eye protection/face protection.
 P301+P312            IF SWALLOWED: Call a POISON CENTER or doctor/physician if you feel unwell.
 P302+P352            IF ON SKIN: Wash with plenty of soap and water.
 P304+P340            IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.
 P305+P351+P338     IF IN EYES: Rinse cautiously with waster for several minutes. Remove contact lenses if present and easy to
                        do. Continue rinsing.
 P362               Take off contaminated clothing and wash before reuse.
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)

 HMIS CLASSIFICATION:
 Health: 2              Fire: 0                  Reactivity Hazard: 0
 NFPA RATING:
 Health: 2            Flammability: 0         Reactivity Hazard: 0

 EYE CONTACT: Causes irritation of the eyes.
 SKIN CONTACT: Causes slight to mild irritation of the skin.
 INHALATION:  Irritating to the skin, eyes, and respiratory tract.
 INGESTION: Toxicity reduced to the extent that this compound is relatively insoluble. In large amounts may cause vomiting,
 abdominal pain, and diarrhea.


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: YF3

 Molecular Weight: 145.90


 CHEMICAL NAME                                           CAS#                               %


 Yttrium (III) Fluoride                                                     13709-49-4                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under eyelids. A
 victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if irritation
 persists.
 INHALATION: Remove to fresh air and keep at rest.  If breathing is difficult, give oxygen.  If not breathing, give artificial respiration.
 Get medical attention if necessary.
 INGESTION: Seek medical assistance immediately. Keep the victim calm. Give the victim water (only if conscious). Induce
 vomiting only if directed by medical personnel.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Product is not flammable
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use fire fighting measures that suit the surrounding fire.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Hydrogen Fluoride and Yttrium Oxides Hydrogen
 fluoride.

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation. Avoid dust
 formation. Avoid breathing dust. Keep unprotected persons away.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Small spills can be mixed with powdered sodium
 bicarbonate, lime, or calcium carbonate and swept up.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Use with adequate ventilation. Avoid
 contact with skin and eyes. Avoid formation of dust. Handle under a dry atmosphere of air and nitrogen.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Hygroscopic. Store in tightly sealed container.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION
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 EXPOSURE CONTROLS
 Component                 Exposure Limits              Basis                           Entity
 Yttrium                          2.5 mg/m3                 TLV                     ACGIH
                                  2.5 mg/m3                 PEL                   OSHA
 Fluoride                     1 mg/m3                  REL                     NIOSH
                            1 mg/m3                   TLV                     ACGIH
                            1 mg/m3                  PEL                   OSHA
                              3mg/g*                       BEI-U                    ACGIH
                               10mg/g**                     BEI-U                    ACGIH

 TLV: Threshold Limit Value over 8 hours of work.           REL: Recommended Exposure Limit
 PEL: Permissible Exposure Limit                           BEI-U: Biological Exposure Indices in Urine.





 STEL: 7.5 mg/m3 15 min TWA: 2.5 mg/m3 8 hr

 EYE PROTECTION: Wear chemical safety glasses or goggles.
 SKIN PROTECTION: Wear nitrile or rubber gloves, apron, or lab coat.
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator.
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

 COLOR AND FORM: White to off white.
 ODOR: None
 MOLECULAR WEIGHT: 145.90
 BOILING POINT: 2230° C
 MELTING POINT: 1387°C
 SPECIFIC GRAVITY: 4.01
 VAPOR DENSITY: No data available
 SOLUBILITY IN WATER: Insoluble

SECTION 10  STABILITY AND REACTIVITY
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 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Moisture
 INCOMPATIBILITY: Strong acids
 DECOMPOSITION PRODUCTS: Hydrogen fluoride and Yttrium oxides.


SECTION 11 TOXICOLOGICAL DATA

 ACUTE TOXICITY: Intraperitoneal (mammal-species unspecified); LD50: 10 mg/kg. Oral (Rat); TDLo: 44 gm/kg/31 D-I.
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available
 RTECS: ZG3417500

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No data available.

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 Not a dangerous good


SECTION 15  REGULATORY INFORMATION

 TSCA: Listed in the TSCA inventory
 SARA 302/304: Not Listed
 SARA (TITLE 313): Not Listed
 CALIFORNIA PROP. 65: Not Listed


SECTION 16  OTHER INFORMATION

 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, ProChem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE REVISED: 07/26
 REVISION SUMMARY: Fax number removed. Updates to the following Sections #2 Hazard Statement added H302+H312+H332 &
 Precautionary Phrases removed P330. Section #5 – Updated Hazardous Combustion Statement. Section #9 – Updated Color & Form
 Statement. All other details in the document about the product remain unchanged. – Revised by EHS 7/26
 Reviewed/Approved 6/26
 SDS DEPT.
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