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               SAFETY DATA SHEET

 1. SUBSTANCE AND SOURCE IDENTIFICATION

Product Identifier
  SRM Number:  4919I
  SRM Name: Strontium-90 Radioactivity Standard
    Other Means of Identification: Not applicable.

Recommended Use of This Material and Restrictions of Use
This Standard Reference Material (SRM) is intended primarily for the calibration of instruments that are used to
measure radioactivity and for the monitoring of radiochemical procedures. A unit of SRM 4919I consists of 5 mL of
1 M (4 %) hydrochloric acid in which a certified quantity of radioactive strontium-90 is dissolved.

Company Information
     National Institute of Standards and Technology
     Standard Reference Materials Program
     100 Bureau Drive, Stop 2300
      Gaithersburg, Maryland 20899-2300

     Telephone: 301-975-2200                         Emergency Telephone ChemTrec:
    FAX: 301-948-3730                                  1-800-424-9300   (North America)
     E-mail: SRMMSDS@nist.gov                        +1-703-527-3887    (International)
     Website: http://www.nist.gov/srm

 2. HAZARDS IDENTIFICATION

Radiological Hazard

Warning:  THIS MATERIAL SHOULD ONLY BE USED BY PERSONS QUALIFIED TO HANDLE
RADIOACTIVE MATERIAL!

SRM 4919I is a radioactive material, strontium-90, with a massic activity of approximately 4 kBq•g-1 in
hydrochloric acid. Strontium-90 decays by beta-particle emission to yittrium-90, which also decays by beta
particle emission.  The beta particles emitted from strontium-90 and yttrium-90 produce bremsstrahlung
photons with energies up to 2 MeV.

This product contains licensed radioactive material and is therefore subject to the requirements of 10 CFR Part 20
(e.g., public and occupational exposure limits, waste disposal). At a minimum, the basic radiation safety principles
of  time,  distance, and  shielding, and  appropriate  radiation  contamination  control  should be  practiced  to
avoid/minimize any external and/or internal exposure. Consult with your Radiation Safety office for your facility’s
radiation safety requirements/precautions specific to the radionuclide(s) (including its activity and chemical/physical
form) in this Radioactive SRM.

Classification
    Physical Hazard: There are no known physical hazards associated with this material.
    Health Hazard:  Skin Corrosion/Irritation         Category 1B
                      Serious Eye Damage/Irritation    Category 1

Label Elements
   Symbol





    Signal Word
   DANGER

   Hazard Statement(s)
   H314               Causes severe skin burns and eye damage.
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    Precautionary Statement(s)
    P260            Do not breathe fumes, mists, vapors, or spray.
    P264             Wash hands thoroughly after handling.
    P280              Wear protective gloves, protective clothing, and eye protection.

   P301+P330+P331      If swallowed: Rinse mouth. Do NOT induce vomiting.
   P303+P361+P353      If on skin (or hair): Remove immediately all contaminated clothing.  Rinse skin with
                           water.
   P304+P340              If inhaled: Remove person to fresh air and keep comfortable for breathing.
   P305+P351+P338      If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if
                           present and easy to do. Continue rinsing.
    P310                Immediately call a doctor.
    P363             Wash contaminated clothing before reuse.

    P405                  Store locked up.

    P501                Dispose of contents and container according to local regulations.

   Hazards Not Otherwise Classified: None.

    Ingredients(s) with Unknown Acute Toxicity: None.

 3. COMPOSITION AND INFORMATION ON HAZARDOUS INGREDIENTS

Substance: Strontium-90 in 1 M hydrochloric acid.

Other Designations:
    Hydrochloric Acid: Muriatic acid; chlorohydric acid; hydrochloride.
    Strontium-90: Not applicable.

The solution also contains trace amounts of yttrium ions (Y+3) and non-radioactive strontium ions (Sr+2). Components
are listed in compliance with OSHA’s 29 CFR 1910.1200; for the actual values see the NIST Certificate.

 Hazardous Component(s)       CAS Number     EC Number     Nominal Mass Concentration
                                               (EINECS)                (%)

 Hydrochloric acid                  7647-01-0           231-595-7                4
 Strontium-90                        not applicable        not applicable                 0.000 000 08
 Non-Hazardous Component(s)
 Water                             7732-18-5           231-791-2               96

 4. FIRST AID MEASURES

Description of First Aid Measures:

    Inhalation:  If adverse effects occur, remove to uncontaminated area. If not breathing, give artificial respiration
    or oxygen by qualified personnel. Seek immediate medical attention.

    Skin Contact: Rinse affected area with copious amounts of water followed by washing with soap and water for
     at least 15 minutes while removing contaminated clothing. Seek medical attention, if needed.

   Eye Contact: Immediately flush eyes, including under the eyelids with copious amounts of water for at least
    30 minutes. Seek immediate medical attention.

    Ingestion: Contact a poison control center immediately for instructions. Wash out mouth with water, but do not
    induce vomiting. Seek medical aid at once, and bring the container or label.

Most Important Symptoms/Effects, Acute and Delayed: Acid burns to skin and eyes.

Indication of any immediate medical attention and special treatment needed, if necessary:  If any of the above
symptoms are present, seek immediate medical attention.

 5. FIRE FIGHTING MEASURES

Fire and Explosion Hazards:  Negligible fire hazard.  See Section 9, “Physical and Chemical Properties” for
flammability properties.
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Extinguishing Media:
     Suitable: Use extinguishing media appropriate to the surrounding fire.
    Unsuitable: None listed.

Specific Hazards Arising from the Chemical: Hydrogen chloride.

Special Protective Equipment and Precautions for Fire-Fighters: Avoid inhalation of material or combustion
byproducts. Wear full protective clothing and NIOSH approved self-contained breathing apparatus (SCBA).

NFPA Ratings: (0 = Minimal; 1 = Slight; 2 = Moderate; 3 = Serious; 4 = Severe)

    Health = 3            Fire = 0          Reactivity = 0

 6. ACCIDENTAL RELEASE MEASURES

This material is radioactive. DO NOT touch spilled material. Immediately notify safety personnel of a spill.

Personal Precautions, Protective Equipment, Methods and Materials for Containment and Clean up:

Radiological Emergency Procedures:
The following is a guide for first responders. The following actions, including remediation, should be carried out by
qualified individuals. In cases where a life-threatening injury occurs concurrent with personal contamination, treat
the injury first.
Do not touch damaged packages or spilled material. Handle as a radioactive material spill. In addition to those actions
described below, the guidelines in the Emergency Response Guidebook (ERG) provide more specific measures that
should be followed.

Spill and Leak Control:
    Alert and clear everyone from the area affected by the spill.
    Take actions to limit the spread of contamination.
   Summon aid.

Damage to the Radioactive Source:
    Evacuate the immediate vicinity around the source.
    Place a barrier at a safe distance from the source.
     Identify area as a radiation hazard.

Suggested Emergency Protective Equipment:
    Gloves
    Footwear Covers
    Outer layer or easily removed protective clothing (as situation requires)

 7. HANDLING AND STORAGE

Safe Handling Precautions and Storage: This material is radioactive.  Store and handle in accordance with all
current regulations and standards. See NRC 10 CFR 20 or state regulations. See Section 8, “Exposure Controls and
Personal Protection”.

 8. EXPOSURE CONTROLS AND PERSONAL PROTECTION

Exposure Limits:

Strontium-90:
       ALIinh: 20 μCi or 740 kBq (bone surface). See NRC 10 CFR 20 Appendix B.
       ALIing: 30 μCi or 1.11 MBq (bone surface)
     OSHA: See OSHA 29 CFR and NRC 10 CFR 20.
     ACGIH: See International Commission on Radiological Protection guidelines.

Hydrochloric Acid:
    NIOSH (REL):   7 mg/m3; 5 ppm (Ceiling)
                    75 mg/m3; 50 ppm (IDLH)
    ACGIH (TLV):   3 mg/m3; 2 ppm (Ceiling)
    OSHA (PEL):    7 mg/m3; 5 ppm (Ceiling)

Engineering Controls:  Provide local exhaust or process enclosure ventilation system. Ensure compliance with
applicable exposure limits.

Personal Protection: In accordance with OSHA 29 CFR 1910.132, subpart I, wear appropriate Personal Protective
Equipment (PPE) to minimize exposure to this material.
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    Respiratory Protection:    If workplace conditions warrant a respirator, a respiratory protection program that
    meets OSHA 29CFR 1910.134 must be followed. Refer to NIOSH 42 CFR 84 for applicable certified respirators.

    Eye/Face Protection: Wear splash resistant safety goggles with a face shield. An eye wash station should be
     readily available near areas of use.

    Skin and Body Protection: Wear protective clothing to prevent contact with skin. Wear appropriate gloves.

 9. PHYSICAL AND CHEMICAL PROPERTIES

   Descriptive Properties:                                         Hydrochloric Acid (4 % of this SRM)

     Appearance (physical state, color, etc.):                          colorless to yellow liquid
     Molecular Formula:                                 HCl
    Molar Mass (g/mol):                                        36.46
    Odor:                                                         not available
    Odor threshold:                                               not available
    pH:                                                <2
     Evaporation rate:                                    >1
     Melting point/freezing point (ºC):                              not available
     Relative Density (g/L) as specific gravity (water = 1):          1 to 1.2
    Vapor Pressure (mmHg):                                      not applicable
    Vapor Density (air = 1):                                        0.7 (water)
      Viscosity (cP):                                         14 mmHg at 20 ºC
      Solubility(ies):                                                 not available
     Partition coefficient (n-octanol/water):                         not available

 Thermal Stability Properties:
     Autoignition Temperature (ºC):                               not applicable
    Thermal Decomposition (ºC):                                  not applicable
      Initial boiling point and boiling range (ºC):                    not available
     Explosive Limits, LEL (Volume %):                           not applicable
     Explosive Limits, UEL (Volume %):                           not applicable
     Flash Point (ºC):                                               not applicable
     Flammability (solid, gas):                                      not applicable

 10. STABILITY AND REACTIVITY

Reactivity:  Stable at normal temperatures and pressure.

      Stability:  X       Stable              Unstable

Possible Hazardous Reactions: None listed.

Conditions to Avoid: Avoid contact with combustible materials and incompatible materials.

Incompatible Materials: Cyanides, metals, amines, bases, metal carbide, oxidizing materials, acids, halo carbons,
combustible materials, halogens, metal salts.

Fire/Explosion Information: See Section 5, “Fire Fighting Measures”.

Hazardous Decomposition: Hydrogen chloride.

Hazardous Polymerization:          Will Occur     X    Will Not Occur

 11. TOXICOLOGICAL INFORMATION

Route of Exposure:    X    Inhalation     X    Skin        X    Ingestion

Symptoms Related to the Physical, Chemical and Toxicological Characteristics:  Burning pain and severe
corrosive skin damage. Permanent eye damage including blindness could result.

Potential Health Effects (Acute, Chronic and Delayed):

   Inhalation: Hydrochloric acid, if inhaled, can damage the mucous membranes and respiratory tract. Short term
   exposure may cause irritation and inflammation of the upper respiratory tract, coughing, choking, sore throat,
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   shortness of breath, headache, dizziness, and nausea. Long term exposure to acid fumes may cause damage to
    teeth, bronchial irritation, chronic cough, bronchial pneumonia, and gastrointestinal disturbances.

   Skin Contact:  Hydrochloric acid can cause severe skin burns.  Severity of the damage depends on the
   concentration and duration of exposure. Effects of acid burns may be delayed.

   Eye Contact:  Hydrochloric acid can cause severe eye irritation, corneal burns, permanent eye damage, or
   blindness. Severity of the damage depends on the concentration and duration of exposure.

   Ingestion: Ingestion of this material is unlikely under normal conditions of use.  If ingested, Hydrochloric acid
   can cause severe burns and damage to the gastrointestinal tract.

Numerical Measures of Toxicity:

   Acute Toxicity:
        Hydrochloric acid,   Rat, Inhalation LC50: 3124 ppm (1 h)
                              Rat, Oral LD50: 238 mg/kg to 277 mg/kg
   Skin Corrosion/Irritation: This SRM contains 4 % hydrochloric acid and it is classified as Category 1.

   Serious Eye Damage/Irritation: This SRM contains 4 % hydrochloric acid and it is classified as Category 1.

   Respiratory Sensitization: No data available.

   Skin Sensitization: No data available.

  Germ Cell Mutagenicity: No data available.

   Carcinogenicity: No data available.

      Listed as a Carcinogen/Potential Carcinogen              Yes       X   No
      Hydrochloric acid is not listed by NTP, IARC or OSHA as a carcinogen/potential carcinogen.

     Radiological Hazard: Strontium-90
     Ionizing radiation is a known carcinogen.

   Reproductive Toxicity: Not classified.
        Hydrochloric acid:   Rat, Inhalation TCLo: 450 mg/kg (1 h, prior to copulation 1 d)

   Specific Target Organ Toxicity, Single Exposure: No data available.

   Specific Target Organ Toxicity, Repeated Exposure: No data available.

   Aspiration Hazard: No data available.

 12. ECOLOGICAL INFORMATION

Ecotoxicity Data:
   Component: Hydrochloric Acid
     Fish Toxicity: Mosquitofish (Gambusia affinis) LC50 (static): 282 mg/L (96 h)
      Invertebrate: Shore crab (Carcinus maenas) LC50 (mortality): 240 mg/L (48 h)
   Component: Strontium-90
   No ecotoxicity data listed.

Persistence and Degradability: No data available.

Bioaccumulative Potential: No data available.

Mobility in Soil: No data available.

Other Adverse Effects: No data available.

 13. DISPOSAL CONSIDERATIONS

Waste Disposal: This material is radioactive. Dispose in accordance with all applicable federal, state, and local
regulations for RADIOACTIVE materials. See NRC 10 CFR 20 subpart K.

 14. TRANSPORTATION INFORMATION

U.S. DOT and IATA:
    Primary Risk: UN2910, Radioactive Material Excepted Package, Hazard Class 7, PG II.
    Subsidiary Risk: Hydrochloric acid, Class 8, PG II; Excepted quantity: E2.
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 15. REGULATORY INFORMATION

U.S. Regulations:

  CERCLA Sections 102a/103 (40 CFR 302.4): Hydrochloric acid, 5000 lbs (2270 kg) final RQ.

  SARA Title III Section 302 (40 CFR 355.30): Hydrochloric acid, 500 lbs (227 kg) TPQ (gas only).

  SARA Title III Section 304 (40 CFR 355.40): Hydrochloric acid, 5000 lbs (2270 kg) EPCRA RQ (gas only).

  SARA Title III Section 313 (40 CFR 372.65): Hydrochloric acid, 1.0 % de minimis concentration

         (acid aerosols including mists, vapors, gas, fog, and other airborne forms of any particle size).

  OSHA Process Safety (29 CFR 1910.119): Not regulated.

  SARA Title III Sections 311/312 Hazardous Categories (40 CFR 370.21):

       ACUTE HEALTH:       Yes.
       CHRONIC HEALTH:    No.
         FIRE:                 No.
        REACTIVE:           No.
        PRESSURE:           No.

State Regulations:
    California Proposition 65: No components are regulated.

U.S. TSCA Inventory: Hydrochloric acid is listed.

TSCA 12(b), Export Notification: No components are listed.

Canadian Regulations:
   WHMIS Information: Not provided for this material.

 16. OTHER INFORMATION

Issue Date: 26 June 2015

Sources: ChemAdvisor, Inc., SDS Hydrochloric Acid, 20 March 2015.

       CDC; NIOSH; NIOSH Pocket Guide  to Chemical Hazards; Department  of Health and Human
          Services (DHHS), Centers for Disease Control and Prevention (CDC), National Institute for Safety and
          Health; Hydrochloric Acid, 18 November 2010; available at http://www.cdc.gov/niosh/npg/npgd0447.html
          (accessed June 2015).

         United States National Library of Medicine, Hazardous Substance Database (HSDB), Hydrochloric Acid;
          available at http://toxnet.nlm.nih.gov/newtoxnet/hsdb.htm (accessed June 2015).

      OSHA 29 CFR, Subpart Z, Ionizing radiation, 1910.1096.

      NRC 10 CFR 20, Standards for Protection Against Radiation.

      DOT 49 CFR 173, Shippers General Requirements for Shipments and Packages.
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Key of Acronyms:

 ACGIH       American Conference of Governmental Industrial    NIOSH        National Institute for Occupational Safety and
                 Hygienists                                                        Health
 ALI          Annual Limit on Intake                       NIST          National Institute of Standards and Technology
 CAS         Chemical Abstracts Service                NRC          Nuclear Regulatory Commission
 CEN         European Committee for Standardization         NTP           National Toxicology Program
 CERCLA     Comprehensive Environmental Response,        OSHA         Occupational Safety and Health Administration
               Compensation, and Liability Act
 CFR         Code of Federal Regulations                  PEL           Permissible Exposure Limit
 CPSU        Coal Mine Dust Personal Sample Unit          RCRA        Resource Conservation and Recovery Act
 DOT         Department of Transportation                REL         Recommended Exposure Limit
 EC50          Effective Concentration, 50 %             RM           Reference Material
 EINECS      European Inventory of Existing Commercial       RQ            Reportable Quantity
               Chemical Substances
 EPCRA      Emergency Planning and Community Right-to-Know  RTECS        Registry of Toxic Effects of Chemical Substances
               Act
 IARC          International Agency for Research on Cancer      SARA        Superfund Amendments and Reauthorization Act
 IATA          International Air Transportation Agency         SCBA         Self-Contained Breathing Apparatus
 IDLH         Immediately Dangerous to Life and Health       SRM          Standard Reference Material
 ISO            International Organization for Standardization      STEL          Short Term Exposure Limit
 LC50          Lethal Concentration, 50 %                   TDLo         Toxic Dose Low
 LD50          Lethal Dose, 50 %                       TLV          Threshold Limit Value
 LEL         Lower Explosive Limit                     TPQ          Threshold Planning Quantity
 MSDS         Material Safety Data Sheet                  TSCA         Toxic Substances Control Act
 NFPA         National Fire Protection Association          TWA        Time Weighted Average
 MSHA       Mine Safety and Health Administration          UEL         Upper Explosive Limit
                                           WHMIS      Workplace Hazardous Materials Information System





Disclaimer:  Physical and chemical data contained in  this SDS are provided only for use in assessing the
hazardous nature of this material. The SDS was prepared carefully, using current references; however, NIST does
not certify the data in the SDS.  The certified values for this material are given in the NIST Certificate.

Users of this SRM should ensure that the SDS in their possession is current. This can be accomplished by contacting
the SRM Program: telephone (301) 975-2200; fax (301) 948-3730; e-mail srmmsds@nist.gov; or via the Internet at
http://www.nist.gov/srm.
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