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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Praseodymium (III) Oxalate Hydrate

 PRODUCT NUMBER:  2977

 CAS NUMBER:        28877-86-3

 SYNONYMS:        Praseodymium oxalate, oxalic acid praseodymium salt.

 MANUFACTURER:


 Prochem, Inc.                                         PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                    IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION


 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Warning

 Hazard Statements

 H315               Causes skin irritation
 H319               Causes serious eye irritation
 H335             May cause respiratory irritation

 Precautionary Phrases


 P261                 Avoid breathing dust/fume/gas/mist/vapors/spray.
 P264             Wash skin thoroughly after handling.
 P280              Wear protective gloves/protective clothing/eye protection/face protection
 P302+P352            IF ON SKIN: Wash with plenty of soap and water.
 P304+P340            IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.
 P305+P351+P338      IF IN EYES: Rinse cautiously with waster for several minutes. Remove contact lenses if present and easy to
                        do. Continue rinsing.
 P403+P233           Store in a well-ventilated place. Keep container tightly closed

 HMIS CLASSIFICATION:
 Health: 0              Fire: 0                  Reactivity Hazard: 0
 NFPA RATING:
 Health: 0            Flammability: 0         Reactivity Hazard: 0
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)


 EYE CONTACT: May cause moderate to severe irritation of the eyes.
 SKIN CONTACT: May cause moderate to severe irritation to the skin.
 INHALATION: Dust may be severely irritating to the nose, mucous membranes, and respiratory tract.
 INGESTION: May be harmful if swallowed


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Pr2(C2O4)3  � xH2O

 Molecular Weight: 545.88 (anhy.)


 CHEMICAL NAME                                           CAS#                               %


 Praseodymium (III) oxalate hydrate                                         28877-86-3                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. A victim may need
 assistance in keeping their eyelids open. Get immediate medical attention.
 SKIN EXPOSURE: Wash the affected area with water. Remove contaminated clothes if necessary. Seek medical
 assistance if irritation persists.
 INHALATION: Remove to fresh air and keep at rest.  If breathing is difficult, give oxygen.  If not breathing, give artificial
 respiration. Get medical attention if necessary.
 INGESTION: Do NOT induce vomiting. Never give anything by mouth to an unconscious person.  If conscious, wash out mouth
 with water. Get medical attention if necessary.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Not available
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Carbon dioxide, dry powder, or foam.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Carbon oxides and praseodymium oxides

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Small spills can be mixed with vermiculite or sodium
 carbonate and swept up and placed in the proper container for disposal.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Avoid contact with skin and eyes. Use with
 adequate ventilation. Wash thoroughly after using. Keep container closed when not in use. Avoid formation of dusts and aerosols.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Keep away from heat and moisture.

SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EXPOSURE CONTROLS: Contains no substances with occupational exposure limit values.
 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield
 SKIN PROTECTION: Wear nitrile or rubber gloves, and a complete suit protecting against chemicals
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.
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SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES

 COLOR AND FORM: Light green powder
 ODOR: No data available
 MOLECULAR WEIGHT: 545.88 (anhy.)
 BOILING POINT: No data available
 MELTING POINT: No data available
 SPECIFIC GRAVITY: No data available
 VAPOR DENSITY: No data available
 SOLUBILITY: Slightly soluble

SECTION 10  STABILITY AND REACTIVITY

 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Avoid moisture.
 INCOMPATIBILITY: Strong oxidizing agents.
 DECOMPOSITION PRODUCTS: Carbon oxides and praseodymium oxides.


SECTION 11 TOXICOLOGICAL DATA

 ACUTE TOXICITY: Not available
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No data available.

SECTION 13  DISPOSAL CONSIDERATIONS


 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 Not a dangerous good.


SECTION 15  REGULATORY INFORMATION

 TSCA: Listed in the TSCA inventory

 DSCL (EEC): Listed on the DSCL inventory

 SARA 302/304: Not Listed

 SARA 311/312: Chronic Health Hazard

 SARA (TITLE 313): Not Listed

 CALIFORNIA PROP. 65: Not Listed

 WHMIS CANADA: Not Listed

 NEW JERSEY RIGHT TO KNOW COMPONENTS: Praseodymium (III) oxalate hydrate

 PENNSYLVANIA RIGHT TO KNOW COMPONENTS: Praseodymium (III) oxalate hydrate
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SECTION 16  OTHER INFORMATION


 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREPARED: 08/14
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