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 SECTION 1     PRODUCT AND COMPANY INFORMATION
 PRODUCT NAME:    Cerium, chips

 PRODUCT NUMBER:  1399

 CAS NUMBER:        7440-45-1

 SYNONYMS:         Rare earth metal

MANUFACTURER:
 ProChem, Inc.                                        PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                    TOLL FREE:    800-795-8788

                   IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION
 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Danger

 Hazard Statements

 H228               Flammable solid.

 Precautionary Phrases

 P210              Keep away from heat/sparks/open flames/hot surfaces. –No smoking.
 P240                Ground/bond container and receiving equipment.
 P241              Use explosion-proof electrical/ventilating/lighting/equipment.
 P270             Do not eat, drink, or smoke when using this product.
 P280              Wear protective gloves/protective clothing/eye protection/face protection.
 P370+P378             In case of fire: Use dry sand, dry chemical, or alcohol-resistant foam for extinction.

 HMIS CLASSIFICATION:
 Health: 2              Fire: 3                  Reactivity Hazard: 1
 NFPA RATING:
 Health: 2            Flammability: 3         Reactivity Hazard: 1       Special: W

 EYE CONTACT: Oil and dust, if present, may cause slight to mild irritation of the eyes.
 SKIN CONTACT: Dust, if present, may cause slight to mild irritation of the skin.
 INHALATION: Inhalation of any oil free fine dust may be irritating to the nasal cavity, mucous membranes, and respiratory tract.
 INGESTION: Mineral oil may be harmful.
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SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS
 Formula: Ce
 Molecular Weight: 140.12


 CHEMICAL NAME                                           CAS#                               %

 Cerium                                                                  7440-45-1                                               100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under eyelids. A
 victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if irritation
 persists.
 INHALATION: Remove to fresh air and keep at rest. Closely monitor the victim for signs of respiratory problems, such as difficulty in
 breathing, coughing, wheezing, or pain. In such cases, seek immediate medical assistance.
 INGESTION: Seek medical assistance immediately. Keep the victim calm. Give the victim water (only if conscious). Induce
 vomiting only if directed by medical personnel.

SECTION 5   FIREFIGHTING MEASURES
 FLASH POINT: Not available
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Use special powder for metal fires. Do not use water. Contact with water released flammable gases.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Cerium oxide

SECTION 6   ACCIDENTAL RELEASE MEASURES
 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation. Avoid the
 formation of dust. Avoid breathing vapors, mist, gas, or dust. Remove from sources of ignition.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Pick up and arrange disposal without creating dust. Sweep
 up and keep in suitable, closed containers for disposal.

SECTION 7   HANDLING AND STORAGE
 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Use with adequate ventilation. Avoid
 contact with skin and eyes. Avoid formation of dust. Handle under inert gas.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Store away from air, water, and moisture. Store
 under dry inert gas. Protect from humidity and water.


SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION
 EXPOSURE CONTROLS: Contains no substances with occupational exposure limits.
 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield.
 SKIN PROTECTION: Wear nitrile or rubber gloves, apron, or lab coat.
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator.
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES
 COLOR AND FORM: Dark grey chips
 ODOR: None
 MOLECULAR WEIGHT: 140.12
 BOILING POINT: 3433° C
 MELTING POINT: 795° C
 SPECIFIC GRAVITY: 6.67
 VAPOR DENSITY: No data available
 SOLUBILITY IN WATER: Contact with water releases flammable gases
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SECTION 10  STABILITY AND REACTIVITY
 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Contact with water or of any oil free fine dust with air. Heat, flames, & sparks.
 INCOMPATIBILITY: Water, alcohols, oxidizers, oxygen, carbon dioxide, halogens, halocarbons, and acids. Strong Acids,
 halogens, strong oxidizing agents, zinc.
 DECOMPOSITION PRODUCTS: Cerium oxide


SECTION 11 TOXICOLOGICAL DATA

 ACUTE TOXICITY:
        LD50 Oral - Rat - male and female - > 5,000 mg/kh Remarks: (in analogy to similar compounds) Inhalation: No data available
        LC50 Inhalation - Rat - male and female - 4 h - > 5.05 mg/l (OECD Test Guideline 403) Remarks: (in analogy to similar products
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available
 RTECS: Not available

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA
 No data available

SECTION 13  DISPOSAL CONSIDERATIONS
 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA
 UN3078
 Cerium
 Class 4.3
 PG II


 Marine Pollutant: No


SECTION 15  REGULATORY INFORMATION

 TSCA: Listed in the TSCA inventory
 SARA 302/304: Not listed
 SARA 311/312: Acute Health Hazard, Reactivity Hazard
 SARA (TITLE 313): Not listed
 PENNSYLVANIA RIGHT TO KNOW: Cerium, slabs, ingots or rods
 NEW JERSEY RIGHT TO KNOW: Cerium, slabs, ingots or rods
 CALIFORNIA PROP. 65: Not Listed


SECTION 16  OTHER INFORMATION
 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, ProChem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE REVISED: 02/24
 SDS DEPT.
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