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               SAFETY DATA SHEET

 1. SUBSTANCE AND SOURCE IDENTIFICATION

Product Identifier
  SRM Number:    4239a
  SRM Name:      Strontium-90 Radioactivity Standard
    Other Means of Identification: Not applicable.

Recommended Use of This Material and Restrictions of Use
    This Standard Reference Material (SRM) is intended primarily for the calibration of instruments that are used to
    measure radioactivity and for the monitoring of radiochemical procedures. A unit of SRM 4239a consists of
    approximately 5 mL of 1 M (3.6 %) hydrochloric acid solution in which a certified amount of Strontium-90 is
    dissolved.

Company Information
     National Institute of Standards and Technology
     Standard Reference Materials Program
     100 Bureau Drive, Stop 2300
      Gaithersburg, Maryland 20899-2300

     Telephone: 301-975-2200                         Emergency Telephone ChemTrec:
     E-mail: SRMMSDS@nist.gov                         1-800-424-9300   (North America)
     Website: https://www.nist.gov/srm                    +1-703-527-3887    (International)


 2. HAZARDS IDENTIFICATION

Radiological Hazard

Warning:  THIS MATERIAL SHOULD ONLY BE USED BY PERSONS QUALIFIED TO HANDLE
RADIOACTIVE MATERIAL!

This product contains licensed radioactive material and is therefore subject to the requirements of 10 CFR Part 20
(e.g., public and occupational exposure limits, waste disposal). At a minimum, the basic radiation safety principles
of  time,  distance, and  shielding, and  appropriate  radiation  contamination  control  should be  practiced  to
avoid/minimize any external and/or internal exposure. Consult with your Radiation Safety office for your facility’s
radiation safety requirements/precautions specific to the radionuclide(s) (including its activity and chemical/physical
form) in this Radioactive SRM.

SRM 4239a is a radioactive material, Strontium-90, with a massic activity of approximately 29.5 kBq•g-1 in a
hydrochloric acid solution. Strontium-90 decays by beta-particle emission to yttrium-90, which also decays by
beta-particle emission. The beta particles emitted from strontium-90 and yttrium-90 produce bremsstrahlung
photons with energies up to 2 MeV.

Classification
    Physical Hazard: There are no known physical hazards associated with this material.
    Health Hazard:  Skin Corrosion/Irritation         Category 1B
                      Serious Eye Damage/Irritation    Category 1

Label Elements
   Symbol





    Signal Word
   DANGER
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   Hazard Statement(s)
   H314               Causes severe skin burns and eye damage.

    Precautionary Statement(s)
    P260            Do not breathe fumes, mists, vapors, or spray.
    P264             Wash hands thoroughly after handling.
    P280              Wear protective gloves, protective clothing, and eye protection.

   P301+P330+P331      If swallowed: Rinse mouth. Do NOT induce vomiting.
   P303+P361+P353      If on skin (or hair): Remove immediately all contaminated clothing.  Rinse skin with
                           water.
   P304+P340              If inhaled: Remove person to fresh air and keep comfortable for breathing.
   P305+P351+P338      If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if
                           present and easy to do. Continue rinsing.
    P310                Immediately call a doctor.
    P363             Wash contaminated clothing before reuse.

    P405                 Store locked up.

    P501                Dispose of contents and container according to local regulations.

   Hazards Not Otherwise Classified: None.

    Ingredients(s) with Unknown Acute Toxicity: None.

 3. COMPOSITION AND INFORMATION ON HAZARDOUS INGREDIENTS

Substance: Strontium-90 in 1 M Hydrochloric Acid.

Other Designations:
    Hydrochloric Acid: Muriatic acid, chlorohydric acid, hydrochloride.
    Strontium-90: Not applicable.

This material contains trace amounts of Y+3 and Sr+2. Components are listed in compliance with OSHA’s 29 CFR
1910.1200; for the actual values see the NIST Certificate.

 Hazardous Component(s)       CAS Number     EC Number     Nominal Mass Concentration
                                               (EINECS)                (%)

 Hydrochloric Acid                  7647-01-0           231-595-7                    3.6
 Strontium-90                    Not applicable      Not applicable                0.000 000 6
 Non-Hazardous Component(s)
 Water                             7732-18-5           231-791-2              >96

 4. FIRST AID MEASURES

Description of First Aid Measures:

    Inhalation:  If adverse effects occur, remove to uncontaminated area. If not breathing, give artificial respiration
    or oxygen by qualified personnel. Seek immediate medical attention.

    Skin Contact: Rinse affected area with copious amounts of water followed by washing with soap and water for
     at least 15 minutes while removing contaminated clothing. Seek medical attention, if needed.

   Eye Contact: Immediately flush eyes, including under the eyelids with copious amounts of water for at least
    30 minutes. Seek immediate medical attention.

    Ingestion: Contact a poison control center immediately for instructions. Wash out mouth with water, but do not
    induce vomiting. Seek medical aid at once, and bring the container or label.

Most Important Symptoms/Effects, Acute and Delayed: Acid burns to skin and eyes.

Indication of any immediate medical attention and special treatment needed, if necessary:  If any of the above
symptoms are present, seek immediate medical attention.
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 5. FIRE FIGHTING MEASURES

Fire and Explosion Hazards:  Negligible fire hazard.  See Section 9, “Physical and Chemical Properties” for
flammability properties.

Extinguishing Media:
     Suitable: Use extinguishing media appropriate to the surrounding fire.
    Unsuitable: None listed.

Specific Hazards Arising from the Chemical: Hydrogen chloride.

Special Protective Equipment and Precautions for Fire-Fighters: Avoid inhalation of material or combustion
byproducts. Wear full protective clothing and NIOSH approved self-contained breathing apparatus (SCBA).


 6. ACCIDENTAL RELEASE MEASURES

This material is radioactive. DO NOT touch spilled material. Immediately notify safety personnel of a spill.

Personal Precautions, Protective Equipment, Methods and Materials for Containment and Clean up:

Radiological Emergency Procedures:
The following is a guide for first responders. The following actions, including remediation, should be carried out by
qualified individuals. In cases where a life-threatening injury occurs concurrent with personal contamination, treat
the injury first.
Do not touch damaged packages or spilled material. Handle as a radioactive material spill. In addition to those actions
described below, the guidelines in the Emergency Response Guidebook (ERG) provide more specific measures that
should be followed.

Spill and Leak Control:
    Alert and clear everyone from the area affected by the spill.
    Take actions to limit the spread of contamination.
   Summon aid.

Damage to the Radioactive Source:
    Evacuate the immediate vicinity around the source.
    Place a barrier at a safe distance from the source.
     Identify area as a radiation hazard.

Suggested Emergency Protective Equipment:
    Gloves
    Footwear Covers
    Outer layer or easily removed protective clothing (as situation requires)

 7. HANDLING AND STORAGE

Safe Handling Precautions and Storage: This material is radioactive.  Store and handle in accordance with all
current regulations and standards. See NRC 10 CFR 20 or state regulations. See Section 8, “Exposure Controls and
Personal Protection”.

 8. EXPOSURE CONTROLS AND PERSONAL PROTECTION

Exposure Limits:

Strontium-90:
       ALIinh: 20 μCi or 740 kBq (bone surface). See NRC 10 CFR 20 Appendix B
       ALIing: 30 μCi or 1.11 MBq (bone surface).
     OSHA: See OSHA 29 CFR and NRC 10 CFR 20.
     ACGIH: See International Commission on Radiological Protection guidelines

Hydrochloric Acid:
     NIOSH (REL):   7 mg/m3; 5 ppm (Ceiling)
                    75 mg/m3; 50 ppm (IDLH)
    ACGIH (TLV):   3 mg/m3; 2 ppm (Ceiling)
    OSHA (PEL):    7 mg/m3; 5 ppm (Ceiling)

Engineering Controls:  Provide local exhaust or process enclosure ventilation system. Ensure compliance with
applicable exposure limits.
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Personal Protection: In accordance with OSHA 29 CFR 1910.132, subpart I, wear appropriate Personal Protective
Equipment (PPE) to minimize exposure to this material.

   Respiratory Protection:  If workplace conditions warrant a respirator, a respiratory protection program that meets
  OSHA 29CFR 1910.134 must be followed.  Refer to NIOSH 42 CFR 84 for applicable certified respirators.

   Eye/Face Protection: Wear splash resistant safety goggles with a face shield. An eye wash station should be
   readily available near areas of use.

   Skin and Body Protection: Wear protective clothing to prevent contact with skin. Wear appropriate gloves.


 9. PHYSICAL AND CHEMICAL PROPERTIES

   Descriptive Properties:

     Appearance (physical state, color, etc.):                        not available
     Molecular Formula:                                           not applicable
    Molar Mass (g/mol):                                          not applicable
    Odor:                                                         not available
    Odor threshold:                                               not available
    pH:                                                           not available
     Evaporation rate (ether = 1):                                   not available
     Melting point/freezing point (ºC):                              not available
     Relative Density (g/L) as specific gravity (water = 1):            not available
    Vapor Pressure (mmHg):                                      not applicable
    Vapor Density (air = 1):                                        0.7 (water)
      Viscosity (cP):                                                 not available
      Solubility(ies):                                                 not available
     Partition coefficient                                           not available
     (n-octanol/water):
      Particle Size:                                                  not applicable

 Thermal Stability Properties:
     Autoignition Temperature (ºC):                               not applicable
    Thermal Decomposition (ºC):                                  not applicable
      Initial boiling point and boiling range (ºC):                    not available
     Explosive Limits, LEL (Volume %):                           not applicable
     Explosive Limits, UEL (Volume %):                           not applicable
     Flash Point (ºC):                                              not applicable
     Flammability (solid, gas):                                     not applicable

 10. STABILITY AND REACTIVITY

Reactivity:  This material is stable at normal temperatures and pressure.

 Stability:     X       Stable              Unstable

Possible Hazardous Reactions: None listed.

Conditions to Avoid: Avoid contact with combustible materials and incompatible materials.

Incompatible Materials: Cyanides, metals, amines, bases, metal carbide, oxidizing materials, acids, halo carbons,
combustible materials, halogens, metal salts.

Fire/Explosion Information: See Section 5, “Fire Fighting Measures”.

Hazardous Decomposition: Hydrogen chloride.

 Hazardous Polymerization:         Will Occur     X    Will Not Occur


 11. TOXICOLOGICAL INFORMATION

 Route of Exposure:   X    Inhalation     X   Skin        X    Ingestion
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Symptoms Related to the Physical, Chemical and Toxicological Characteristics:  Burning pain and severe
corrosive skin damage. Permanent eye damage including blindness could result.

Potential Health Effects (Acute, Chronic and Delayed):

   Inhalation: Hydrochloric acid, if inhaled, can damage the mucous membranes and respiratory tract. Short term
   exposure may cause irritation and inflammation of the upper respiratory tract, coughing, choking, sore throat,
   shortness of breath, headache, dizziness, and nausea. Long term exposure to acid fumes may cause damage to
    teeth, bronchial irritation, chronic cough, bronchial pneumonia, and gastrointestinal disturbances.

   Skin Contact:  Hydrochloric acid can cause severe skin burns.  Severity of the damage depends on the
   concentration and duration of exposure. Effects of acid burns may be delayed.

   Eye Contact:  Hydrochloric acid can cause severe eye irritation, corneal burns, permanent eye damage, or
   blindness. Severity of the damage depends on the concentration and duration of exposure.

   Ingestion: Ingestion of this material is unlikely under normal conditions of use.  If ingested, Hydrochloric acid
   can cause severe burns and damage to the gastrointestinal tract.

Numerical Measures of Toxicity:

   Acute Toxicity:
        Hydrochloric acid,   Rat, Inhalation LC50: 3124 ppm (1 h)
                              Rat, Oral LD50: 238 - 277 mg/kg
   Skin Corrosion/Irritation: This SRM contains 3.6 % Hydrochloric acid and it is classified as Category 1.

   Serious Eye Damage/Eye Irritation:  This SRM contains 3.6 % Hydrochloric acid and  it is classified as
   Category 1.

   Respiratory Sensitization: No data available.

   Skin Sensitization: No data available.

  Germ Cell Mutagenicity: No data available.

   Carcinogenicity: No data available.

      Listed as a Carcinogen/Potential Carcinogen              Yes       X   No
      Hydrochloric acid is not listed by NTP, IARC or OSHA as a carcinogen.

     Radiological Hazard: Strontium-90
     Ionizing radiation is a known carcinogen.

   Reproductive Toxicity: Not classified.
        Hydrochloric acid:   Rat, Inhalation TCLo: 450 mg/kg (1 h, prior to copulation 1 d)

   Specific Target Organ Toxicity, Single Exposure: No data available.

   Specific Target Organ Toxicity, Repeated Exposure: No data available.

   Aspiration Hazard: No data available.

 12. ECOLOGICAL INFORMATION

Ecotoxicity Data:
   Component: Hydrochloric Acid
     Fish Toxicity: Mosquitofish (Gambusia affinis) LC50 (static): 282 mg/L (96 h)
      Invertebrate: Shore crab (Carcinus maenas) LC50 (mortality): 240 mg/L (48 h)
   Component: Strontium-90
   No ecotoxicity data listed.

Persistence and Degradability: No data available.

Bioaccumulative Potential: No data available.

Mobility in Soil: No data available.

Other Adverse Effects: No data available.
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 13. DISPOSAL CONSIDERATIONS

Waste Disposal: This material is radioactive. Dispose in accordance with all applicable federal, state, and local
regulations for RADIOACTIVE materials. See NRC 10 CFR 20 subpart K.

 14. TRANSPORTATION INFORMATION

U.S. DOT and IATA:
   Primary Risk: UN2910, Radioactive Material Excepted Package, Hazard Class 7.
    Subsidiary Risk: Hydrochloric Acid, Excepted Quantity E2.

 15. REGULATORY INFORMATION

U.S. Regulations:

  CERCLA Sections 102a/103 (40 CFR 302.4): Hydrochloric acid, 5000 lbs (2270 kg) final RQ.

  SARA Title III Section 302 (40 CFR 355.30): Hydrochloric acid, 500 lbs (227 kg) TPQ (gas only).

  SARA Title III Section 304 (40 CFR 355.40): Hydrochloric acid, 5000 lbs (2270 kg) EPCRA RQ (gas only).

  SARA Title III Section 313 (40 CFR 372.65): Hydrochloric acid, 1.0 % de minimis concentration

         (acid aerosols including mists, vapors, gas, fog, and other airborne forms of any particle size).

  OSHA Process Safety (29 CFR 1910.119): Not regulated.

  SARA Title III Sections 311/312 Hazardous Categories (40 CFR 370.21):

       ACUTE HEALTH:       Yes.
       CHRONIC HEALTH:    No.
         FIRE:                 No.
        REACTIVE:           No.
        PRESSURE:           No.

State Regulations:
    California Proposition 65: No components are regulated.

U.S. TSCA Inventory: Hydrochloric acid listed.

TSCA 12(b), Export Notification: No components are listed.

Canadian Regulations:
   WHMIS Information: Not provided for this material.

 16. OTHER INFORMATION

Issue Date: 11 October 2022

Sources: ChemAdvisor, Inc., SDS Hydrochloric Acid, 20 March 2015.

       CDC; NIOSH; NIOSH Pocket Guide  to Chemical Hazards; Department  of  Health and Human
          Services (DHHS), Centers for Disease Control and Prevention (CDC), National Institute for Safety and
          Health; Hydrochloric Acid, 18 November 2010; available https://www.cdc.gov/niosh/npg/npgd0332.html
          (accessed Oct 2022).

        PubChem,  United   States  National  Library  of  Medicine,  Hydrochloric  Acid;   available   at
         https://pubchem.ncbi.nlm.nih.gov/compound/313 (accessed Oct 2022).

      OSHA 29 CFR, Subpart Z, Ionizing radiation, 1910.1096.

      NRC 10 CFR 20, Standards for Protection Against Radiation.

      DOT 49 CFR 173, Shippers General Requirements for Shipments and Packages.
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Key of Acronyms:

 ACGIH       American Conference  of Governmental  Industrial NIST          National Institute of Standards and Technology
                 Hygienists
 ALI          Annual Limit on Intake                   NRC          Nuclear Regulatory Commission
 CAS          Chemical Abstracts Service                  NTP           National Toxicology Program
 CEN          European Committee for Standardization         OSHA         Occupational Safety and Health Administration
 CERCLA      Comprehensive      Environmental      Response, PEL           Permissible Exposure Limit
                Compensation, and Liability Act
 CFR         Code of Federal Regulations                RCRA        Resource Conservation and Recovery Act
 CPSU         Coal Mine Dust Personal Sample Unit           REL         Recommended Exposure Limit
 DOT          Department of Transportation             RM           Reference Material
 EC50           Effective Concentration, 50 %               RQ            Reportable Quantity
 EINECS       European Inventory of Existing Commercial Chemical RTECS        Registry of Toxic Effects of Chemical Substances
                 Substances
 EPCRA       Emergency Planning and Community Right-to-Know SARA        Superfund Amendments and Reauthorization Act
               Act
 IARC           International Agency for Research on Cancer      SCBA         Self-Contained Breathing Apparatus
 IATA           International Air Transportation Agency         SRM          Standard Reference Material
 IDLH          Immediately Dangerous to Life and Health         STEL          Short Term Exposure Limit
 ISO             International Organization for Standardization      TDLo         Toxic Dose Low
 LC50           Lethal Concentration, 50 %                 TLV          Threshold Limit Value
 LD50          Lethal Dose, 50 %                        TPQ          Threshold Planning Quantity
 LEL         Lower Explosive Limit                    TSCA         Toxic Substances Control Act
 MSDS          Material Safety Data Sheet               TWA        Time Weighted Average
 MSHA       Mine Safety and Health Administration          UEL         Upper Explosive Limit
 NIOSH         National Institute for Occupational Safety and Health  WHMIS      Workplace Hazardous Materials Information System





Disclaimer:  The NIST SDS information is specific to the NIST product and is believed to be correct, based upon
our current knowledge. The SDS may not necessarily be all inclusive and should be used only as a guide. NIST does
not guarantee the accuracy or completeness of this information. The only official source for specific values and
uncertainties is the certificate or report.

Users of this SRM should ensure that the SDS in their possession is current. This can be accomplished by contacting
the SRM  Program:  telephone  (301)  975-2200;  e-mail  srmmsds@nist.gov;  or  via  the   Internet   at
https://www.nist.gov/srm.
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