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 SECTION 1     PRODUCT AND COMPANY INFORMATION

 PRODUCT NAME:    Cerium (III) Nitrate Hexahydrate

 PRODUCT NUMBER:  1423

 CAS NUMBER:        10294-41-4

 SYNONYMS:         Cerous nitrate hexahydrate, nitric acid, cerium (3+) salt

 MANUFACTURER:


 Prochem, Inc.                                         PHONE:        815-398-1788
 826 Roosevelt Road                                          FAX:           815-398-1810
 Rockford, IL  61109                                     TOLL FREE:    800-795-8788

                    IN CASE OF TRANSPORTATION EMERGENCY CONTACT CHEM-TREC: 1-800-424-9300

SECTION 2    HAZARDS IDENTIFICATION


 CLASSIFICATION OF SUBSTANCE OR MIXTURE

 Pictogram


 Signal Word         Danger

 Hazard Statements

 H272             May intensify fire, oxidizer.
 H318               Causes serious eye damage.


 Precautionary Phrases

 P210              Keep away from heat.
 P220                 Keep/Store away from clothing/combustible materials.
 P221               Take any precaution to avoid mixing with combustibles.
 P280              Wear protective gloves/protective clothing/eye protection/face protection.
 P305+P351+P338      IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to
                        do. Continue rinsing.
 P310                 Immediately call a POISON CENTER or doctor/physician.
 P370+P378             In case of fire: Use dry sand, dry chemical, or alcohol-resistant foam for extinction.

 HMIS CLASSIFICATION:
 Health: 2            Chronic: *               Fire: 0                     Reactivity Hazard: 2
 NFPA RATING:
 Health: 2            Flammability: 0         Reactivity Hazard: 2       Special: OX
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SECTION 2    HAZARDS IDENTIFICATION (Cont.)


 EYE CONTACT: Causes slight to mild irritation of the eyes.
 SKIN CONTACT: Causes slight to mild irritation of the skin.
 INHALATION:  Irritating to the nose, mucous membranes, and respiratory tract.
 INGESTION: Ingestion may lead to dizziness, abdominal cramps, vomiting, bloody diarrhea, weakness, and convulsions.


SECTION 3      COMPOSITION / INFORMATION ON INGREDIENTS

 Formula: Ce(NO3)3 � 6H2O

 Molecular Weight: 434.22


 CHEMICAL NAME                                           CAS#                               %


 Cerium (III) Nitrate Hexahydrate                                            10294-41-4                                             100

SECTION 4   FIRST AID MEASURES

 EYE EXPOSURE: Immediately flush the eyes with copious amounts of water for at least 15 minutes. Assure flushing under
 eyelids. A victim may need assistance in keeping their eyelids open. Get immediate competent medical attention.
 SKIN EXPOSURE: Wash affected area with water. Remove contaminated clothes if necessary. Seek medical assistance if
 irritation persists.
 INHALATION: Remove to fresh air and keep at rest. Closely monitor the victim for signs of respiratory problems, such as
 difficulty in breathing, coughing, wheezing, or pain. In such cases, seek immediate medical assistance.
 INGESTION: Seek medical assistance immediately. Keep the victim calm. Give the victim water (only if conscious). Induce
 vomiting only if directed by medical personnel.

SECTION 5   FIREFIGHTING MEASURES

 FLASH POINT: Contact with combustible material may cause fire.
 AUTO IGNITION TEMPERATURE: Not available
 EXPLOSION LIMITS: Not available
 EXTINGUISHING MEDIUM: Carbon dioxide, extinguishing powder, or water spray. Fight large fires with water spray or alcohol
 resistant foam. This substance is an oxidizer and its heat of reaction with reducing agents or combustibles may cause ignition.
 SPECIAL FIRE FIGHTING PROCEDURES: Wear self-contained, approved breathing apparatus and full protective clothing,
 including eye protection and boots.
 HAZARDOUS COMBUSTION AND DECOMPOSITION PRODUCTS: Nitrogen oxides and cerium oxides.

SECTION 6   ACCIDENTAL RELEASE MEASURES

 PERSONAL PRECAUTIONS: Wear all appropriate equipment when using this material. Ensure adequate ventilation. Avoid the
 formation of dust. Avoid breathing vapors, mist, gas, or dust.
 ENVIRONMENTAL PRECAUTIONS: Prevent spillage from entering drains or allowing to be released into the environment.
 METHODS AND MATERIALS FOR CONTAINMENT AND CLEANING UP: Pick up and arrange disposal without creating dust. Sweep
 up and keep in suitable, closed containers for disposal.

SECTION 7   HANDLING AND STORAGE

 PRECAUTIONS FOR SAFE HANDLING: Wear appropriate personal protective equipment. Use with adequate ventilation. Avoid
 contact with skin and eyes. Avoid formation of dust. Keep away from heat and sources of ignition.
 CONDITIONS FOR SAFE STORAGE: Store in cool, dry, and well-ventilated area. Store under inert gas. Air sensitive. Hygroscopic.
 Store away from flammable substances, reducing agents, metal powders, water, and moisture. Do not store with organic materials.
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SECTION 8  EXPOSURE CONTROLS AND PERSONAL PROTECTION

 EXPOSURE CONTROLS: Contains no substances with occupational exposure limit values.
 EYE PROTECTION: Wear chemical safety glasses or goggles and face shield.
 SKIN PROTECTION: Wear nitrile or rubber gloves, apron, or lab coat.
 VENTILATION: Provide local exhaust, preferably mechanical.
 RESPIRATOR: Use an approved respirator.
 ADDITIONAL PROTECTION: Provide eyewash stations, quick-drench showers and washing facilities accessible to areas of use and
 handling.

SECTION 9 PHYSICAL AND CHEMICAL PROPERTIES


 COLOR AND FORM: White to yellow solid
 ODOR: None
 MOLECULAR WEIGHT: 434.22
 BOILING POINT: No data available
 MELTING POINT: 65° C
 SPECIFIC GRAVITY: No data available
 VAPOR DENSITY: No data available
 SOLUBILITY: Vary soluble

SECTION 10  STABILITY AND REACTIVITY

 STABILITY: Stable
 HAZARDOUS POLYMERIZATION: Will not occur
 CONDITIONS TO AVOID: Hygroscopic. Air sensitive.
 INCOMPATIBILITY: Strong reducing agents and strong acids.
 DECOMPOSITION PRODUCTS: Nitrogen oxides and cerium oxides.


SECTION 11 TOXICOLOGICAL DATA


 ACUTE TOXICITY: LD50 Oral – rat – 4,200 mg/kg.
 CARCINOGENIC EFFECTS: No components of this product present at levels greater than or equal to 0.1% is identified a carcinogen.
 MUTAGENIC EFFECTS: Not available
 TETRATOGENIC EFFECTS: Not available
 RTECS: FK6300000

 To the best of our knowledge the toxicological effects of this compound have not been fully investigated.

SECTION 12  ECOLOGICAL DATA

 No data available

SECTION 13  DISPOSAL CONSIDERATIONS

 Dispose of in according to local, state, and federal regulations.

SECTION 14  TRANSPORTATION DATA

 UN1477                                        Marine Pollutant: No

 Nitrates, inorganic, n.o.s.

 (Cerium (III) Nitrate Hexahydrate)

 Class 5.1

 PG II
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SECTION 15  REGULATORY INFORMATION

 TSCA: Not listed in the TSCA inventory

 SARA 302/304: Not listed

 SARA 311/312: Reactivity Hazard, Acute Health Hazard, Chronic Health Hazard

 SARA (TITLE 313): Not listed

 PENNSYLVANIA RIGHT TO KNOW: Cerium (III) nitrate hexahydrate

 NEW JERSEY RIGHT TO KNOW: Cerium (III) nitrate hexahydrate

 CALIFORNIA PROP. 65: Not Listed


SECTION 16  OTHER INFORMATION

 DISCLAIMER: The information herein is believed to be accurate and reliable as of the date compiled. However, Prochem, Inc.
 makes no representation, warranty, or guarantee of any kind with respect to the information in this document or any use of the
 product based on the information.
 DATE PREPARED: 12/14
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