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 ALFAA40123

  Zirconium(IV) oxide, 18% in H2O, colloidal dispersion, stabilized with 1.3%
                                yttrium oxide

   SECTION 1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING


产品说明:产品说明:产品说明:产品说明:                氧化锆(IV)氧化锆(IV)氧化锆(IV)氧化锆(IV)
Product Description:               Zirconium(IV) oxide, 18% in H2O, colloidal dispersion, stabilized with 1.3% yttrium
                                 oxide

Cat No. :                        40123
Molecular Formula               ZrO2 /Y2 O3

Supplier                         Avocado Research Chemicals Ltd.
                                        (Part of Thermo Fisher Scientific)
                                 Shore Road, Heysham
                                     Lancashire, LA3 2XY,
                                    United Kingdom
                                        Office Tel: +44 (0) 1524 850506
                                        Office Fax: +44 (0) 1524 850608


Emergency Telephone Number     For information US call: 001-800-227-6701 / Europe call: +32 14 57 52 11
                               Emergency Number US:001-201-796-7100 / Europe: +32 14 57 52 99
                         CHEMTREC Tel. No. US:001-800-424-9300 / Europe:001-703-527-3887

E-mail address                    begel.sdsdesk@thermofisher.com

Recommended Use                 Laboratory chemicals.
Uses advised against           No Information available

                           SECTION 2. HAZARD IDENTIFICATION


            Physical State                      Appearance                          Odor
             Liquid dispersion                No information available              No information available

                                        Emergency Overview
          Causes serious eye damage. Causes skin irritation. May be corrosive to metals. May be harmful if inhaled.


Classification of the substance or mixture

Substances/mixtures corrosive to metal                                              Category 1
Acute Inhalation Toxicity - Vapors                                                   Category 5
Skin Corrosion/Irritation                                                           Category 2
Serious Eye Damage/Eye Irritation                                                  Category 1

Label Elements
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Signal Word                    Danger

Hazard Statements
H290 - May be corrosive to metals
H318 - Causes serious eye damage
H315 - Causes skin irritation
H333 - May be harmful if inhaled

Precautionary Statements
Prevention
P234 - Keep only in original packaging
P264 - Wash face, hands and any exposed skin thoroughly after handling
P271 - Use only outdoors or in a well-ventilated area
P280 - Wear protective gloves/protective clothing/eye protection/face protection
Response
P302 + P352 - IF ON SKIN: Wash with plenty of soap and water
P304 + P340 - IF INHALED: Remove person to fresh air and keep comfortable for breathing
P305 + P351 + P338 - IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to
do. Continue rinsing
P310 - Immediately call a POISON CENTER or doctor
P362 + P364 - Take off contaminated clothing and wash it before reuse
P390 - Absorb spillage to prevent material damage
Storage
P406 - Store in corrosion resistant polypropylene container with a resistant inliner
Disposal
P501 - Dispose of contents/ container to an approved waste disposal plant

Physical and Chemical Hazards
May be corrosive to metals.
Health Hazards
Corrosive. Causes eye burns. Causes skin irritation. Causes serious eye damage. May be harmful if inhaled.
Environmental hazards
Contains no substances known to be hazardous to the environment or not degradable in waste water treatment plants. Will likely
be mobile in the environment due to its water solubility. The product is water soluble, and may spread in water systems.
No information available
This product does not contain any known or suspected endocrine disruptors. Toxic to terrestrial vertebrates.

                  SECTION 3. COMPOSITION/INFORMATION ON INGREDIENTS


                           Component                              CAS No                Weight %
                                  Water                                            7732-18-5                    77.7
                                 Zirconium oxide                                        1314-23-4                   18.00
                              Nitricacid…% [C≤70%]                                  7697-37-2                    3.00
                                 Yttrium oxide (Y2O3)                                      1314-36-9                      1.3



                            SECTION 4. FIRST AID MEASURES


General Advice
If symptoms persist, call a physician.

Eye Contact
Rinse immediately with plenty of water, also under the eyelids, for at least 15 minutes. Get medical attention.

Skin Contact
Wash off immediately with plenty of water for at least 15 minutes. If skin irritation persists, call a physician.

Inhalation
Remove to fresh air. If not breathing, give artificial respiration. Get medical attention if symptoms occur.

Ingestion
______________________________________________________________________________________________
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Clean mouth with water and drink afterwards plenty of water.

Most important symptoms and effects
None reasonably foreseeable. Causes severe eye damage.


Self-Protection of the First Aider
Ensure that medical personnel are aware of the material(s) involved, take precautions to protect themselves and prevent spread of
contamination.

Notes to Physician
Treat symptomatically.

                          SECTION 5. FIRE-FIGHTING MEASURES


Suitable Extinguishing Media
Not combustible.

Extinguishing media which must not be used for safety reasons
No information available.

Specific Hazards Arising from the Chemical
Thermal decomposition can lead to release of irritating gases and vapors.


Protective Equipment and Precautions for Firefighters
As in any fire, wear self-contained breathing apparatus pressure-demand, MSHA/NIOSH (approved or equivalent) and full
protective gear.

                       SECTION 6. ACCIDENTAL RELEASE MEASURES


Personal Precautions
Ensure adequate ventilation. Use personal protective equipment as required.


Environmental Precautions
Should not be released into the environment. Do not allow material to contaminate ground water system. Do not flush into surface
water or sanitary sewer system.


Methods for Containment and Clean Up
Soak up with inert absorbent material. Keep in suitable, closed containers for disposal.


Refer to protective measures listed in Sections 8 and 13.

                          SECTION 7. HANDLING AND STORAGE


Handling
Wear personal protective equipment/face protection. Ensure adequate ventilation. Do not get in eyes, on skin, or on clothing. Avoid
ingestion and inhalation.

Storage
Keep container tightly closed in a dry and well-ventilated place.

Specific Use(s)
Use in laboratories

                  SECTION 8. EXPOSURE CONTROLS/PERSONAL PROTECTION

Control Parameters

______________________________________________________________________________________________
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      Component                China              ACGIH TLV           OSHA PEL              NIOSH
      Zirconium oxide                            -               TWA: 5 mg/m3         (Vacated) TWA: 5 mg/m3        IDLH: 25 mg/m3
                                                    STEL: 10 mg/m3       (Vacated) STEL: 10 mg/m3   REL = 5 mg/m3 (TWA)
                                                                                                   STEL: 10 mg/m3
  Nitricacid…% [C≤70%]                   -                TWA: 2 ppm           (Vacated) TWA: 2 ppm          IDLH: 25 ppm
                                                     STEL: 4 ppm          (Vacated) TWA: 5 mg/m3     REL = 2 ppm (TWA)
                                                                                    (Vacated) STEL: 4 ppm    REL = 5 mg/m3 (TWA)
                                                                                  (Vacated) STEL: 10 mg/m3        STEL: 4 ppm
                                                                     TWA: 2 ppm            STEL: 10 mg/m3
                                                                    TWA: 5 mg/m3
    Yttrium oxide (Y2O3)                         -               TWA: 1 mg/m3                                     IDLH: 500 mg/m3
                                                                                   REL = 1 mg/m3 (TWA)

      Component            Hong Kong                Thailand            European Union       The United Kingdom
      Zirconium oxide                            -               TWA: 5 mg/m3                                STEL: 10 mg/m3 15 min
                                                                                       TWA: 5 mg/m3 8 hr
  Nitricacid…% [C≤70%]      TWA: 2 ppm            TWA: 2 ppm          STEL: 1 ppm (15min)       STEL: 1 ppm 15 min
                         TWA: 5.2 mg/m3                              STEL: 2.6 mg/m3 (15min)    STEL: 2.6 mg/m3 15 min
                              STEL: 4 ppm
                             STEL: 10 mg/m3

Legend

ACGIH - American Conference of Governmental Industrial Hygienists
OSHA - Occupational Safety and Health Administration
NIOSH: NIOSH - National Institute for Occupational Safety and Health

Monitoring methods
MDHS 91 Metals and metalloids in workplace air by X-ray fluorescence spectrometry MDHS 99 Metals in air by ICP-AES

Exposure Controls

Engineering Measures
Ensure that eyewash stations and safety showers are close to the workstation location. Wherever possible, engineering control
measures such as the isolation or enclosure of the process, the introduction of process or equipment changes to minimise release
or contact, and the use of properly designed ventilation systems, should be adopted to control hazardous materials at source.

Personal protective equipment

   Eye Protection                Goggles (European standard - EN 166)

   Hand Protection                  Protective gloves

    Glove material     Breakthrough time  Glove thickness   EU standard             Glove comments
      Natural rubber     See manufacturers               -          EN 374             (minimum requirement)
        Nitrile rubber       recommendations
       Neoprene
       PVC
Inspect gloves before use.
Please observe the instructions regarding permeability and breakthrough time which are provided by the supplier of the gloves.
(Refer to manufacturer/supplier for information)
Ensure gloves are suitable for the task: Chemical compatability, Dexterity, Operational conditions, User susceptibility, e.g.
sensitisation effects, also take into consideration the specific local conditions under which the product is used, such as the danger
of cuts, abrasion.
Remove gloves with care avoiding skin contamination.

   Skin and body protection       Long sleeved clothing

   Respiratory Protection       When workers are facing concentrations above the exposure limit they must use
                                      appropriate certified respirators.
                              To protect the wearer, respiratory protective equipment must be the correct fit and be used
                               and maintained properly

   Large scale/emergency use    Use a NIOSH/MSHA or European Standard EN 136 approved respirator if exposure limits
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                                    are exceeded or if irritation or other symptoms are experienced
                           Recommended Filter type: Particulates filter conforming to EN 143

   Small scale/Laboratory use     Use a NIOSH/MSHA or European Standard EN 149:2001 approved respirator if exposure
                                              limits are exceeded or if irritation or other symptoms are experienced.
                           Recommended half mask:- Particle filtering: EN149:2001
                           When RPE is used a face piece Fit Test should be conducted


Hygiene Measures                Handle in accordance with good industrial hygiene and safety practice.

Environmental exposure controls  No information available.

                     SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES


Appearance
Physical State                        Liquid dispersion

Odor                       No information available
Odor Threshold               No data available
pH                         No information available
Melting Point/Range            No data available
Softening Point                No data available
Boiling Point/Range            No information available
Flash Point                   No information available           Method - No information available
Evaporation Rate              No data available
Flammability (solid,gas)            Not applicable                         Liquid
Explosion Limits               No data available

Vapor Pressure                  23 hPa @ 20 °C
Vapor Density                 No data available                         (Air = 1.0)
Specific Gravity  / Density        No data available
Bulk Density                      Not applicable                         Liquid
Water Solubility                      Miscible
Solubility in other solvents       No information available
Partition Coefficient (n-octanol/water)
Component                        log Pow
Nitricacid…% [C≤70%]            -2.3
Autoignition Temperature        No data available
Decomposition Temperature      No data available
Viscosity                    No data available
Explosive Properties            No information available
Oxidizing Properties            No information available


Molecular Formula               ZrO2 /Y2 O3



                         SECTION 10. STABILITY AND REACTIVITY


Stability                             Stable under normal conditions.

Hazardous Reactions            None under normal processing.
Hazardous Polymerization        No information available.

Conditions to Avoid             None known.

Materials to avoid              No information available.


Hazardous Decomposition Products Nitrogen oxides (NOx). Metal oxides.
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                        SECTION 11. TOXICOLOGICAL INFORMATION


Product Information

(a) acute toxicity;
Toxicology data for the components

           Component                    LD50 Oral                LD50 Dermal             LC50 Inhalation
                Water                                               -                                            -                                            -
             Zirconium oxide                                                               LC50 > 4.3 mg/L  ( Rat ) 4 h

         Nitricacid…% [C ≤70%]                                                          LC50 = 2500 ppm. (Rat) 1h
           Yttrium oxide (Y2O3)                                                             LC50 > 5.09 mg/L  ( Rat ) 4 h


(b) skin corrosion/irritation;        Category 2


(c) serious eye damage/irritation;   Category 1


(d) respiratory or skin sensitization;
   Respiratory                No data available
   Skin                     No data available

(e) germ cell mutagenicity;       No data available

(f) carcinogenicity;             No data available

                                 There are no known carcinogenic chemicals in this product



(g) reproductive toxicity;         No data available


(h) STOT-single exposure;        No data available



(i) STOT-repeated exposure;      No data available

   Target Organs               None known.


(j) aspiration hazard;            No data available

Symptoms  / effects,both acute and No information available
delayed

                         SECTION 12. ECOLOGICAL INFORMATION


Ecotoxicity effects              May cause long-term adverse effects in the environment. Do not allow material to
                                   contaminate ground water system.


           Component                Freshwater Fish         Water Flea        Freshwater Algae         Microtox
             Zirconium oxide             LC50: > 100 mg/L, 96h
                                                      static (Danio rerio)



Persistence and Degradability      Product contains heavy metals. Discharge into the environment must be avoided. Special
                                      pre-treatment is necessary
______________________________________________________________________________________________
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   Persistence                  based on information available, May persist.
   Degradation in sewage          Contains substances known to be hazardous to the environment or not degradable in waste
   treatment plant                 water treatment plants.


Bioaccumulative Potential        May have some potential to bioaccumulate

           Component                                 log Pow                           Bioconcentration factor (BCF)
         Nitricacid…% [C ≤70%]                                -2.3                            No data available


Mobility in soil                  The product is water soluble, and may spread in water systems Will likely be mobile in the
                                   environment due to its water solubility Highly mobile in soils


Endocrine Disruptor Information    This product does not contain any known or suspected endocrine disruptors
Persistent Organic Pollutant        This product does not contain any known or suspected substance
Ozone Depletion Potential           This product does not contain any known or suspected substance

                         SECTION 13. DISPOSAL CONSIDERATIONS


Waste from Residues/Unused      Waste is classified as hazardous. Dispose of in accordance with the European Directives
Products                        on waste and hazardous waste. Dispose of in accordance with local regulations.

Contaminated Packaging           Dispose of this container to hazardous or special waste collection point.

Other Information                Waste codes should be assigned by the user based on the application for which the product
                             was used. Do not empty into drains. Do not flush to sewer.

                         SECTION 14. TRANSPORT INFORMATION


Road and Rail Transport

UN-No                       UN1760
Proper Shipping Name          CORROSIVE LIQUID, N.O.S.
   Technical Shipping Name         Nitric acid solution
Hazard Class                    8
Packing Group                                     III


IMDG/IMO

UN-No                       UN1760
Proper Shipping Name          CORROSIVE LIQUID, N.O.S.
   Technical Shipping Name         Nitric acid solution
Hazard Class                    8
Packing Group                                     III


IATA

UN-No                       UN1760
Proper Shipping Name          CORROSIVE LIQUID, N.O.S.
   Technical Shipping Name         Nitric acid solution
Hazard Class                    8
Packing Group                                     III


Special Precautions for User      No special precautions required

                         SECTION 15. REGULATORY INFORMATION
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International Inventories
China, X = listed, Australia, U.S.A. (TSCA), Canada (DSL/NDSL), Europe (EINECS/ELINCS/NLP), Australia (AICS), Korea (KECL), China (IECSC),
Japan (ENCS), Philippines (PICCS), Taiwan (TCSI), Japan (ISHL), New Zealand (NZIoC), Japan (ISHL).

    Component        The        List of    IECSC   EINECS   TSCA   DSL   PICCS  ENCS    ISHL    AICS    KECL
                     Inventory of dangerous
                   Hazardous  goods GB
                    Chemicals   12268 -
                        (2015      2012
                         Edition)
       Water                    -                 -        X      231-791-2    X      X      X      X             X     KE-35400
   Zirconium oxide             -                 -        X      215-227-2    X      X      X      X      X      X     KE-35630
Nitricacid…% [C≤70    X        X       X      231-714-2    X      X      X      X      X      X     KE-25911
        %]
 Yttrium oxide (Y2O3)          -                 -        X      215-233-5    X      X      X      X      X      X     KE-35504



National Regulations


                            SECTION 16. OTHER INFORMATION


Prepared By                         Health, Safety and Environmental Department
Revision Date                     05-Aug-2026
Revision Summary            SDS sections updated.

Training Advice
Chemical hazard awareness training, incorporating labelling, Safety Data Sheets (SDS), Personal Protective Equipment (PPE) and
hygiene.
Use of personal protective equipment, covering appropriate selection, compatibility, breakthrough thresholds, care, maintenance, fit
and standards.
First aid for chemical exposure, including the use of eye wash and safety showers.

                                              Legend

CAS - Chemical Abstracts Service                          TSCA - United States Toxic Substances Control Act Section 8(b)
                                                                       Inventory
EINECS/ELINCS - European Inventory of Existing Commercial Chemical DSL/NDSL - Canadian Domestic Substances List/Non-Domestic
Substances/EU List of Notified Chemical Substances                  Substances List
PICCS - Philippines Inventory of Chemicals and Chemical Substances  ENCS - Japanese Existing and New Chemical Substances
IECSC - Chinese Inventory of Existing Chemical Substances          AICS - Australian Inventory of Chemical Substances
KECL - Korean Existing and Evaluated Chemical Substances         NZIoC - New Zealand Inventory of Chemicals


WEL - Workplace Exposure Limit                        TWA - Time Weighted Average
ACGIH - American Conference of Governmental Industrial Hygienists   IARC - International Agency for Research on Cancer
DNEL - Derived No Effect Level                           PNEC - Predicted No Effect Concentration
RPE - Respiratory Protective Equipment                        LD50 - Lethal Dose 50%
LC50 - Lethal Concentration 50%                            EC50 - Effective Concentration 50%
NOEC - No Observed Effect Concentration                 POW - Partition coefficient Octanol:Water
PBT - Persistent, Bioaccumulative, Toxic                       vPvB - very Persistent, very Bioaccumulative


ICAO/IATA - International Civil Aviation Organization/International Air   IMO/IMDG - International Maritime Organization/International Maritime
Transport Association                                          Dangerous Goods Code
ADR - European Agreement Concerning the International Carriage of   MARPOL - International Convention for the Prevention of Pollution from
Dangerous Goods by Road                                         Ships
OECD - Organisation for Economic Co-operation and Development    ATE - Acute Toxicity Estimate
BCF - Bioconcentration factor                           VOC - (Volatile Organic Compound)

Key literature references and sources for data
https://echa.europa.eu/information-on-chemicals
Suppliers safety data sheet, Chemadvisor - LOLI, Merck index, RTECS
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Physical hazards              On basis of test data
Health Hazards                       Calculation method
Environmental hazards              Calculation method




                                                    Disclaimer
 The information provided in this Safety Data Sheet is correct to the best of our knowledge, information and belief at the
 date of its publication. The information given is designed only as a guidance for safe handling, use, processing, storage,
   transportation, disposal and release and is not to be considered a warranty or quality specification. The information
relates only to the specific material designated and may not be valid for such material used in combination with any other
                                 materials or in any process, unless specified in the text

                    End of Safety Data Sheet





______________________________________________________________________________________________
                                              Page 9
